|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Source: Document 5A/TEMP/9 | **Annex 15 to****Document 5A/79-E** |
| **1 June 2012** |
| **English only** |
| Annex 15 to Working Party 5A Chairman’s Report |
| working document to a Preliminary DRAFT REVISION OF RECOMMENDATION ITU-R M.1801-1[[1]](#footnote-1)\* |
| Radio interface standards for broadband wireless access systems, including mobile and nomadic applications, in the mobile service operating below 6 GHz |

(Questions ITU‑R 212/5 and ITU‑R 238/5)

(2007-2010)

# 1 Introduction

This Recommendation recommends specific standards for broadband wireless access[[2]](#footnote-2) in the mobile service. These specific standards are composed of common specifications developed by standards development organizations (SDOs). Using this Recommendation, manufacturers and operators should be able to determine the most suitable standards for their needs.

These standards support a wide range of applications in urban, suburban and rural areas for both generic broadband internet data and real-time data, including applications such as voice and videoconferencing.

# 2 Scope

This Recommendation identifies specific radio interface standards for BWA systems in the mobile service operating below 6 GHz. The standards included in this Recommendation are capable of supporting users at broadband data rates, taking into account the ITU‑R definitions of “wireless access” and “broadband wireless access” found in Recommendation ITU‑R F.1399[[3]](#footnote-3).

This Recommendation is not intended to deal with the identification of suitable frequency bands for BWA systems, nor with any regulatory issues.

# 3 Related ITU Recommendations

The existing Recommendations that are considered to be of importance in the development of this particular Recommendation are as follows:

[Recommendation ITU-R F.1399](http://www.itu.int/rec/R-REC-F.1399/en) – Vocabulary of terms for wireless access.

[Recommendation ITU-R F.1763](http://www.itu.int/rec/R-REC-F.1763/en) – Radio interface standards for broadband wireless access systems in the fixed service operating below 66 GHz.

[Recommendation ITU-R M.1678](http://www.itu.int/rec/R-REC-M.1678/en) – Adaptive antennas for mobile systems.

# 4 Acronyms and abbreviations

AA Adaptive antenna

ACK Acknowledgement (channel)

AN Access network

ARIB Association of Radio Industries and Businesses

ARQ Automatic repeat request

AT Access terminal

ATIS Alliance for Telecommunications Industry Solutions

ATM Asynchronous transfer mode

BCCH Broadcast control channel

BER Bit-error ratio

BRAN Broadband radio access network

BS Base station

BSR Base station router

BTC Block turbo code

BWA Broadband wireless access

CC Convolutional coding

CDMA Code division multiple access

CDMA-MC Code division multiple access – multi carrier

CL Connection layer

C-plane Control plane

CS-OFDMA Code spread OFDMA

CTC Convolutional turbo code

DECT Digital enhanced cordless telecommunications

DLC Data link control

DS-CDMA Direct-sequence code division multiple access

DSSS Direct sequence spread spectrum

E-DCH Enhanced dedicated channel

EGPRS Enhanced general packet radio service

EPC Evolved packet core

ETSI European Telecommunication Standards Institute

EV-DO Evolution data optimized

FC Forward channel

FCC Forward control channel

FDD Frequency division duplex

FEC Forward-error correction

FER Frame error rate

FHSS Frequency hopping spread spectrum

FT Fixed termination

GERAN GSM edge radio access network

GoS Grade of service

GPRS General packet radio service

GPS Global positioning system

HC-SDMA High capacity-spatial division multiple access

HiperLAN High performance RLAN

HiperMAN High performance metropolitan area network

HRPD High rate packet data

HSDPA High speed downlink packet access

HS-DSCH High speed downlink shared channel

HSUPA High speed uplink packet access

IEEE Institute of Electrical and Electronics Engineers

IETF Internet Engineering Task force

IP Internet protocol

LAC Link access control

LAN Local area network

LDPC Low density parity check

LLC Logic link control

MAC Medium access control

MAN Metropolitan area network

MCSB Multi-carrier synchronous beamforming

MIMO Multiple input multiple output

MS Mobile station

NLoS Non-line-of-sight

OFDM Orthogonal frequency-division multiplexing

OFDMA Orthogonal frequency-division multiple access

OSI Open systems interconnection

PDCP Packet data convergence protocol

PHS Personal handyphone system

PHY Physical layer

PLP Physical layer protocol

PT Portable termination

QAM Quadrature amplitude modulation

QoS Quality-of-service

RAC Reverse access channel

RF Radio frequency

RLAN Radio local area network

RLC Radio link control

RLP Radio link protocol

RTC Reverse traffic channel

SC Single carrier

SC-FDMA Single carrier-frequency division multiple access

SCG Subcarrier group

SDMA Spatial division multiple access

SDO Standards development organization

SISO Single input single output

SL Security/session/stream layer

SM Spatial multiplexing

SNP Signalling network protocol

TCC Traffic code channels

TDD Time-division duplex

TDMA Time-division multiple access

TDMA-SC TDMA-single carrier

TD-SCDMA Time-division-synchronized CDMA

TTA Telecommunications Technology Association

U-plane User plane

WiBro Wireless broadband

WirelessMAN Wireless metropolitan area network

WTSC Wireless Technologies and Systems Committee

WWINA Wireless wideband Internet access

XGP eXtended Global Platform

# 5 Noting

Recommendation ITU‑R F.1763 recommends radio interface standards for broadband wireless access systems in the fixed service operating below 66 GHz.

The ITU Radiocommunication Assembly,

*recommends*

**1** that the radio interface standards in Annexes 1 to 7 should be used for BWA systems in the mobile service operating below 6 GHz.

NOTE 1 – Annex 8 provides a summary of the characteristics of the standards found in Annexes 1 to 7.

**Annex 1

(no change)**

**Annex 2

(no change)**

**Annex 3

(no change)**

**Annex 4

ATIS WTSC radio interface standard for BWA systems
in the mobile service**

# 1 ATIS WTSC wireless wideband internet access standard

The Wireless Technologies and Systems Committee (WTSC) of the Alliance of Telecommunications Industry Solutions (ATIS), an American National Standards Institute (ANSI)‑accredited standards development organization, has developed an American National Standard that adheres to its adopted requirements for wireless wideband internet access (WWINA) systems. The WWINA air interface standard enables wireless portability and nomadic roaming subscriber services that complement the DSL and cable modem markets. This system is optimized for high-speed packet data services that operate on a separate, data-optimized channel. The WWINA requirements specify a non-line-of-sight wireless internet air interface for full-screen, full-performance multimedia devices.

This air interface provides for portable access terminal (AT) devices with improved performance when compared to other systems that are targeted for high-mobility user devices. More specifically, the WWINA air interface optimizes the following performance attributes:

– system data speeds;

– system coverage/range;

– network capacity;

– minimum network complexity;

– grade-of-service and quality-of-service management.

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |
|  |  |

# 42 ATIS-0700004.2005 high capacity-spatial division multiple access (HC-SDMA)

## 42.1 Overview of the radio interface

The HC-SDMA standard specifies the radio interface for a wide-area mobile broadband system. HC-SDMA uses TDD and adaptive antenna (AA) technologies, along with multi-antenna spatial processing algorithms to produce a spectrally efficient mobile communications system that can provide a mobile broadband service deployed in as little as a single (unpaired) 5 MHz band of spectrum licensed for mobile services. HC-SDMA systems are designed to operate in licensed spectrum below 3 GHz, which is the best suited for mobile applications offering full mobility and wide area coverage. Because it is based on TDD technology and does not require symmetrical paired bands separated by an appropriate band gap or duplexer spacing, systems based on the HC‑SDMA standard can easily be re-banded for operation in different frequency bands. The HC‑SDMA technology achieves a channel transmission rate of 20 Mbit/s in a 5 MHz licensed band. With its frequency re-use factor of *N* = 1/2, in a deployment using 10 MHz of licensed spectrum the 40 Mbit/s transmission rate is fully available in every cell in an HC-SDMA network, which is a spectral efficiency of 4 bits/s/Hz/cell.

## 42.2 Detailed specifications of the radio interface

The HC-SDMA air interface has a TDD/TDMA structure whose physical and logical characteristics have been chosen for the efficient transport of end-user IP data and to extract maximum benefit from adaptive antenna processing. The physical aspects of the protocol are arranged to provide spatial training data, and correlated uplink and downlink interference environments, for logical channels amenable to directive transmission and reception such as traffic channels. Conversely, channels not amenable to directive processing, such as paging and broadcast channels have smaller payloads and receive a greater degree of error protection to balance their links with those of the directively processed channels. Adaptive modulation and channel coding, along with uplink and downlink power control, are incorporated to provide reliable transmission across a wide range of link conditions. Modulation, coding and power control are complemented by a fast ARQ to provide a reliable link. Fast, low-overhead make-before-break inter-cell handover is also supported. Authentication, authorization, and privacy for the radio access link is provided by mutual authentication of the terminals and access network, and by encryption.

The HC-SDMA air interface has three layers designated as L1, L2, and L3.

Table 1 describes the air interface functionality embodied in each layer. Each layer’s features are briefly described below; more detailed overviews of key aspects are described in subsequent sections of this document.

TABLE 1

**Air interface layers**

|  |  |
| --- | --- |
| **Layer** | **Defined properties** |
| L1 | Frame and burst structures, modulation and channel coding, timing advance |
| L2 | Reliable transmission, logical to physical channel mapping, bulk encryption |
| L3 | Session management, resource management, mobility management, fragmentation, power control, link adaptation, authentication |

Table 2 summarizes the key elements of the HC-SDMA air interface.

TABLE 2

**Summary of the basic elements of the HC-SDMA air interface**

|  |  |
| --- | --- |
| **Quantity** | **Value** |
| Duplex method | TDD |
| Multiple access method | FDMA/TDMA/SDMA |
| Access scheme | Collision sense/avoidance, centrally scheduled |
| Carrier spacing | 625 kHz |
| Frame period | 5 ms |
| User data rate asymmetry | 3:1 down:up asymmetry at peak rates |
| Uplink time-slots | 3 |
| Downlink time-slots | 3 |
| Range | > 15 km |
| Symbol rate | 500 kbaud/sec |
| Pulse shaping | Root raised cosine |
| Excess channel bandwidth | 25% |
| Modulation and coding | – Independent frame-by-frame selection of uplink and downlink constellation + coding– 8 uplink constellation + coding classes– 9 downlink constellation + coding classes– Constant modulus and rectangular constellations |
| Power control | Frame-by-frame uplink and downlink open and closed loop  |
| Fast ARQ | Yes |
| Carrier and time-slot aggregation | Yes |
| QoS | DiffServ (Differentiated services) policy specification, supporting rate limiting, priority, partitioning, etc. |
| Security | Mutual AT and BSR authentication, encryption for privacy |
| Handover | AT directed, make-before-break |
| Resource allocation | Dynamic, bandwidth on demand |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |
|  |  |

All The standard referenced in this annex is available in electronic form at: <https://www.atis.org/docstore/default.aspx>.

**Annex 5

(no change)**

**Annex 6

(no change)**

**Annex 7

(no change)**

**Annex 8

Key characteristics of standards**

Table 7 provides a summary of key characteristics of each standard.

TABLE 7

**Key technical parameters**

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| IEEE 802.16 WirelessMAN/ETSI HiperMAN(Annex 3) | Flexible from 1.25 MHz up to 28 MHz.Typical bandwidths are:3.5, 5, 7, 8.75, 10 and20 MHz | Up:– QPSK-1/2, 3/4– 16-QAM-1/2, 3/4 – 64-QAM-1/2, 2/3,  3/4, 5/6Down:– QPSK-1/2, 3/4– 16-QAM-1/2, 3/4 – 64-QAM-1/2, 2/3,  3/4, 5/6 | CC/CTCOther options:BTC/LDPC | Up to 17.5 Mbit/s with SISOUp to 35 Mbit/s with (2 × 2) MIMOUp to 70 Mbit/s with (4 × 4) MIMO | Yes | Yes | TDD/FDD/HFDD | OFDMATDMA | 5 msOther options: 2, 2.5, 4, 8, 10, 12.5 and 20 ms | Mobile |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |

TABLE 7 (*continued*)

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ATIS-0700004.2005 high capacity-spatial division multiple access(HC-SDMA) (Annex 4) | 0.625 MHz | Up:– BPSK, QPSK,  8-PSK, 12-QAM,  16-QAM 3/4Down:– BPSK, QPSK,  8-PSK, 12-QAM,  16-QAM,  24-QAM 8/9 | Convolu-tional and block code | Up:2.866 Mbit/s ×8 sub-channels × 4 spatial channels =91.7 Mbit/s Down:2.5 Mbit/s × 8 sub-channels ×4 spatial channels = 80 Mbit/s  | Yes | Yes | TDD | TDMA/FDMA/SDMA | 5 ms | Mobile |
|  |  |  |  |  |  |  |  |  |  |  |
| eXtended Global Platform : XGP(Annex 5) | 1.25 MHz2.5 MHz5 MHz10 MHz20 MHz | Up and down:BPSK 1/2, 2/3QPSK 1/2, 3/416-QAM 1/2, 3/464-QAM 4/6, 5/6256-QAM 6/8, 7/8 | Convolu-tional codeTurbo code (option) | Up:9.85 Mbit/sDown:10.7 Mbit/s(in case of SISO, symmetry) | Yes (option) | Yes (option) | TDD | OFDMA SC-FDMATDMA | 5 ms | Mobile |
| IEEE 802.11-2007 Subclause 18 (Formerly 802.11b) (Annex 1) | 22 MHz | Up and down:DQPSK CCKBPSK PBCC – 1/2QPSK PBCC – 1/2 | Uncoded/ CC | 2.5 Mbit/s | No | No | TDD | CSMA/CA | Variable frame duration | Nomadic |

TABLE 7 (*continued*)

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| IEEE 802.11-2007Subclause 17 (Formerly 802.11a) (Annex 1) | 5 MHz10 MHz20 MHz | Up and down:64-QAM OFDM 2/3, 3/416-QAM OFDM –1/2, 3/4QPSK OFDM – 1/2, 3/4BPSK OFDM – 1/2, 3/4 | CC | 13.5 Mbit/s | No | No | TDD | CSMA/ CA | Variable frame duration | Nomadic |
| IEEE 802.11-2007 Subclause 19 (Formerly 802.11g)(Annex 1) | 20 MHz | Up and down:64-QAM OFDM 2/3, 3/416-QAM OFDM – 1/2, 3/4QPSK OFDM – 1/2, 3/4BPSK OFDM – 1/2, 3/48-PSK PBCC – 2/364-QAM DSSS-OFDM – 2/3, 3/416-QAM DSSS-OFDM – 1/2, 3/4QPSK DSSS-OFDM – 1/2, 3/4BPSK DSSS-OFDM – 1/2, 3/4 | CC | 13.5 Mbit/s | No | No | TDD | CSMA/ CA | Variable frame duration | Nomadic |

TABLE 7 (*continued*)

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| IEEE 802.11-2007As amended by IEEE 802.11n (Subclause 20) (Annex 1)  | 20 MHz40 MHz | Up and down :64-QAM OFDM – 2/3, 3/4, 5/616-QAM OFDM –1/2, 3/4QPSK OFDM – 1/2, 3/4BPSK OFDM – 1/2 | CC and LDPC | 75 Mbit/s | Yes | Yes | TDD | CSMA/CA | Variable frame duration | Nomadic |
| ETSI BRAN HiperLAN 2(Annex 1) | 20 MHz | 64-QAM-OFDM16-QAM-OFDMQPSK-OFDMBPSK-OFDMboth upstream and downstream | CC | 6, 9, 12, 18, 27, 36 and 54 Mbit/s in 20 MHz channel (only 20 MHz channels supported) | No | No | TDD | TDMA | 2 ms | Nomadic |
| ARIB HiSWANa(Annex 1) | 4 × 20 MHz(5.15-5.25 GHz)4 × 20 MHz(4.9-5.0 GHz) | – BPSK 1/2– BPSK 3/4– QPSK 1/2– QPSK 3/4– 16-QAM 9/16– 16-QAM 3/4– 64-QAM 3/4 | Convolu-tional | 6-54 Mbit/s in 20 MHz | No | No | TDD | TDMA | 2 ms | Nomadic |
| IMT-2000 CDMA Direct Spread(Annex 2) | 5 MHz(E-UTRAN) 1.4 MHz, 3 MHz, 5 MHz, 10 MHz, 15 MHz, 20 MHz | Up: QPSK, 16-QAMDown: 16-QAM, QPSK,64-QAM (E-UTRAN) QPSK, 16-QAM, 64-QAM | Convolu-tional turbo | Up:11.5 Mbit/sDown:42 Mbit/s(E-UTRAN)Up: 75.3 Mbit/s / 20 MHz(3)Down: 302.7 Mbit/s / 20 MHz(3) | Yes | Yes | FDD | CDMA(E-UTRAN) OFDM in DLSC-FDMA in UL | 2 ms and 10 ms(E-UTRAN) 10 msSub-frame length 1 ms | Mobile |

TABLE 7 (*continued*)

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| IMT-2000 CDMA Multi-Carrier(Annex 2) | 1.25 MHz and 3.75 MHz(cdma2000)1.25-20 MHz(cdma2000 HRPD) 1.25‑20 MHz, 153.6 kHz granularity(UMB) | Up: BPSK, QPSK,8-PSKDown: QPSK, 8-PSK, 16‑QAM,(cdma2000) QPSK, 8-PSK, 16‑QAM, 64-QAM (cdma2000 HRPD)QPSK, 8-PSK, 16‑QAM, 64-QAM(UMB) | Convolu-tional/ turbo(cdma2000 and cdma2000 HRPD) Convolu-tional/ turbo/ LDPC (optional)(UMB) | Up:1.8 Mbit/s per 1.25 MHz channelDown 3.1 Mbit/sPer 1.25 MHz (cdma2000)Up:1.8 Mbit/sper 1.25 MHz channelDown: 4.9 Mbit/sPer 1.25 MHz channel(cdma2000 HRPD)Up:75 Mbit/s for 20 MHzDown: 228 Mbit/s for 20 MHz(UMB) | No(cdma2000 and cdma2000 HRPD) Yes(UMB) | No(cdma2000 and cdma2000 HRPD)Yes(UMB) | FDD(cdma2000 and cdma2000 HRPD)FDD/TDD(UMB) | CDMA(cdma2000 and cdma2000 HRPD) CDMA and OFDMA(UMB) | Down:1.25, 1.67 2.5, 5, 10, 20, 40, 80 msUp:6.66, 10, 20, 26.67, 40, 80 ms (cdma2000)Down:1.67, 3.33, 6,66,13.33,26.67 Up:1.67, 6.66, 13.33, 20, 26.67(cdma2000 HRPD)Down:0.911 msUp:0.911 ms(UMB) | Mobile |

TABLE 7 (*continued*)

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| IMT-2000 CDMA TDD(Annex 2) | 1.28 Mchip/sTDD option: Less than 1.6 MHz3.84 Mchip/sTDD option: Less than 5 MHz7.68 Mchip/s TDD option:Less than 10 MHz(E-UTRAN) 1.4 MHz, 3 MHz, 5 MHz, 10 MHz, 15 MHz and 20 MHz | 1.28 Mchip/s TDD option:Up: 8‑PSK, QPSK, 16-QAM,Down: 8-PSK, 16-QAM, QPSK3.84 Mchip/sTDD option:Up: 16-QAM, QPSKDown: 16-QAM, QPSK 7.68 Mchip/s TDD option:Up: 16-QAM, QPSK Down: 16-QAM, QPSK(E-UTRAN)QPSK, 16-QAM, 64-QAM | Convolu-tional turbo | 1.28 Mchip/s TDD option:Up: 2.2 Mbit/s / 1.6 MHz(2)Down: 2.8 Mbit/s / 1.6 MHz(2)3.84 Mchip/s TDD option:Up: 9.2 Mbit/s Down: 10.2 Mbit/s7.68 Mchip/s TDD option:Up: 17.7 Mbit/s / 10 MHzDown: 20.4 Mbit/s / 10 MHz(E-UTRAN)Up: 75.3 Mbit/s / 20 MHz(3)Down:302.7 Mbit/s / 20 MHz(3) | Yes | No(E-UTRAN)Yes | TDD | TDMA/CDMA(E-UTRAN) OFDM in DL. SC-FDMA in UL | 1.28 Mchip/s TDD option: 10 msSub-frame length: 5 ms3.84 Mchip/s TDD option: 10 ms7.68 Mchip/s TDD option: 10 ms(E-UTRAN) 10 msSub-frame length: 1 ms | Mobile |

TABLE 7 (*continued*)

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| IMT-2000 TDMA Single-Carrier(Annex 2) | 2 × 200 kHz2 × Dual 200 kHz2 × 1.6 MHz | Up:– GMSK– 8-PSK– QPSK,– 16-QAM, – 32-QAM– B-OQAM– Q-OQAM 0.329 –  1/1Down:– GMSK– 8-PSK– QPSK,– 16-QAM, – 32-QAM– B-OQAM– Q-OQAM 0.329 –  1/1 | Punctured convolu-tional codeTurbo code | Up:16.25 Mbit/s20.312 Mbit/s40.625 Mbit/sDown:16.25 Mbit/s20.312 Mbit/s40.625 Mbit/s | Not explicit but not precluded | Not explicit but not precluded | FDD | TDMA | 4.6 ms4.615 ms | Mobile |
| IMT-2000 FDMA/TDMA(Annex 2) | 1.728 MHz | Up and down:GFSKπ/2-DBPSKπ/4-DQPSKπ/8-D8-PSK16-QAM, 64-QAM | Depends on service:CRC, BCH, Reed-Solomon, Turbo | 20 Mbit/s | Partial | Partial | TDD | TDMA | 10 ms | Mobile |
| IMT-2000 OFDMA TDD WMAN(Annex 2) | 5 MHz,7 MHz,8.75 MHz,10 MHz | Up:– QPSK-1/2, 3/4– 16-QAM-1/2, 3/4– 64-QAM-1/2, 2/3,  3/4, 5/6Down:– QPSK-1/2, 3/4– 16-QAM-1/2, 3/4 – 64-QAM-1/2, 2/3,  3/4, 5/6 | CC/CTCOther options:BTC/LDPC | Up to 17.5 Mbit/s with SISOUp to 35 Mbit/s with (2 × 2) MIMOUp to 70 Mbit/s with (4 × 4) MIMO | Yes | Yes | TDDFDD | OFDMA | 5 ms | Mobile |

TABLE 7 (*end*)

| Standard | Nominal RF channel bandwidth | Modulation/coding rate(1) – upstream – downstream | Coding support | Peak channel transmission rate per 5 MHz channel (except as noted) | Beam-forming support (yes/no) | Support for MIMO (yes/no) | Duplex method | Multiple access method | Frame duration | Mobility capabilities (nomadic/mobile) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| IEEE 802.20(Annex 6) | Flexible from 625 kHz, up to 20 MHz | Wideband mode:Up: QPSK, 8-PSK, 16-QAM, 64-QAMDown: QPSK, 8‑PSK, 16-QAM, 64-QAM625 kHz mode:Pi/2 BPSK, QPSK, 8‑PSK, 12‑QAM, 16‑QAM, 24‑QAM, 32‑QAM, 64‑QAM | Convolu-tional, Turbo, LDPC Code, parity check code, extended Hamming code | Peak rates of 288 Mbit/s DL and 75 Mbit/s UL in 20 MHz | Yes: SDMA, and beam-forming support on forward and reverse links | Yes: Single codeword and multi codeword MIMO support | TDDFDDHFDD | OFDMATDMA/ FDMA/ SDMA | Wideband mode: 0.911 ms  625 kHz mode: 5 ms | Mobile |
| YD/T 1956-2009Air interface of SCDMA broadband wireless access system standard(Annex 7) | Multiple of 1 MHz up to 5 MHz | QPSK, 8-PSK, 16‑QAM, 64‑QAM | Reed-Solomon | 15 Mbit/s in 5 MHz | Yes | Yes | TDD | CS-OFDMA | 10 ms | Mobile |
| (1) Including all applicable modes, or at least the maximum and the minimum. (2) In 5 MHz three 1.28 Mchip/s TDD carriers can be deployed. (3) E-UTRAN supports scalable bandwidth operation up to 20 MHz in both the uplink and downlink. |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \* This Recommendation should be brought to the attention of ITU-T Study Groups 2 and 15. [↑](#footnote-ref-1)
2. “Wireless access” and “BWA” are defined in Recommendation ITU‑R F.1399, which also provides definitions of the terms “fixed”, “mobile” and “nomadic” wireless access. [↑](#footnote-ref-2)
3. *Broadband wireless access* is defined as wireless access in which the connection(s) capabilities are higher than the *primary rate*, which is defined as the transmission bit rate of 1.544 Mbit/s (T1) or 2.048 Mbit/s (E1). *Wireless access* is defined as end-user radio connection(s) to core networks. [↑](#footnote-ref-3)