|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| **PLENARY MEETING** | **Addendum 17 toDocument 8-E** |
|  | **5 June 2015** |
|  | **Original: Russian** |
|  |
| Regional Commonwealth in the field of Communications Common Proposals |
| Proposals for the work of the conference |
|  |
| Agenda item 1.17 |

1.17 to consider possible spectrum requirements and regulatory actions, including appropriate aeronautical allocations, to support wireless avionics intra-communications (WAIC), in accordance withResolution **423 (WRC‑12)**;

Resolution **423 (WRC‑12)**: Consideration of regulatory actions, including allocations, to support Wireless Avionics Intra-Communications

Introduction

The RCC Administrations do not object to the allocation of the radio frequency band 4 200‑4 400 MHz in the aeronautical mobile (R) service for use by WAIC systems only, maintaining the status of the Earth exploration-satellite service (EESS) and space research service (SRS) as passive services and protecting the operation of aeronautical radionavigation services (ARNS) (this corresponds to the method described in the CPM Report).

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD RCC/8A17/1

2 700-4 800 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 4 200-4 400 AERONAUTICAL MOBILE (R) ADD 5.A117 AERONAUTICAL RADIONAVIGATION MOD 5.438 5.439 5.440 ADD 5.B117 |

MOD RCC/8A17/2

5.438 Use of the band 4 200-4 400 MHz by the aeronautical radionavigation service is reserved exclusively for radio altimeters installed on board aircraft and for the associated transponders on the ground.

ADD RCC/8A17/3

5.A117 Use of the frequency band 4 200-4 400 MHz by stations in the aeronautical mobile (R) service is reserved exclusively for wireless avionics intra-communication systems that operate in accordance with recognized international aeronautical standards. Such use shall be in accordance with Resolution **[RCC-A117-WAIC] (WRC‑15)**.

**Reasons:** This footnote makes reference to the following Resolution [RCC-A117-WAIC] (WRC‑15).

ADD RCC/8A17/4

5.B117 Passive sensing in the Earth exploration-satellite and space research services may be authorized in the frequency band 4 200-4 400 MHz on a secondary basis.

SUP RCC/8A17/5

RESOLUTION 423 (WRC‑12)

Consideration of regulatory actions, including allocations, to support
Wireless Avionics Intra-Communications

ADD RCC/8A17/6

DRAFT NEW RESOLUTION [rcc-A117-WAIC] (WRC-15)]

Use of Wireless Avionics Intra-Communications in the
frequency band 4 200-4 400 MHz

The World Radiocommunication Conference (Geneva, 2015),

considering

*a)* that aircraft are designed to enhance efficiency, reliability and safety, as well as to be more environmentally friendly;

*b)* that Wireless Avionics Intra-Communications (WAIC) systems provide radiocommunications between two or more aircraft stations integrated into or installed on a single aircraft, supporting the safe operation of the aircraft;

*c)* that WAIC systems do not provide radiocommunications between an aircraft and the ground, another aircraft or a satellite;

*d)* that WAIC systems operate in a manner that ensures the safe operation of an aircraft;

*e)* that WAIC systems operate during all phases of flight, including on the ground;

*f)* that aircraft equipped with WAIC systems operate globally;

*g)* that WAIC systems operating inside an aircraft receive the benefits of fuselage attenuation to facilitate sharing with other services;

*h)* that Recommendation ITU‑R M.2067 provides technical characteristics and operational objectives for WAIC systems,

recognizing

that Annex 10 to the Convention on International Civil Aviation contains Standards and Recommended Practices (SARPs) for safety aeronautical radionavigation and radiocommunication systems used by international civil aviation,

resolves

1 that WAIC is defined as radiocommunication between two or more aircraft stations located on a single aircraft, supporting the safe operation of the aircraft;

2 that the WAIC systems operating in the frequency band 4 200-4 400 MHz shall not cause harmful interference to, nor claim protection from systems of the aeronautical radionavigation service operating in this frequency band;

3 that the WAIC systems operating in the frequency band 4 200-4 400 MHz shall comply with Standards and Recommended Practices published in Annex 10 to the Convention on International Civil Aviation;

4 that No. **43.1** shall not apply for WAIC systems,

instructs the Secretary-General

to bring this Resolution to the attention of ICAO,

invites ICAO

to take into account Recommendation ITU-R M.[WAIC-CONDITIONS] in the course of development of SARPs for WAIC systems.

**Reasons:** This resolution provides relevant regulatory provisions to satisfy the agenda item.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_