|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15) Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 2 to Document 118(Add.9)-E** |
|  | **19 October 2015** |
|  | **Original: English** |
|  | |
| Indonesia (Republic of), Malaysia | |
| Proposals for the work of the conference | |
|  | |
| Agenda item 1.9.2 | |

1.9 to consider, in accordance with Resolution **758 (WRC‑12)**:

1.9.2 the possibility of allocating the bands 7 375-7 750 MHz and 8 025-8 400 MHz to the maritime-mobile satellite service and additional regulatory measures, depending on the results of appropriate studies;

Introduction

Indonesia and Malaysia oppose the new allocation to MMSS in the band 7 375-7 750 MHz and 8 025‑8 400 MHz. Hence, Indonesia and Malaysia support no change in Radio Regulations. Furthermore, Indonesia and Malaysia also support the suppression of the Resolution 758 (WRC‑12).

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

NOC INS/MLA/118A9A2/1

7 250-8 500 MHz

|  |  |  |
| --- | --- | --- |
| Allocation to services | | |
| Region 1 | Region 2 | Region 3 |
| 7 300-7 450 FIXED  FIXED-SATELLITE (space-to-Earth)  MOBILE except aeronautical mobile  5.461 | | |
| 7 450-7 550 FIXED  FIXED-SATELLITE (space-to-Earth)  METEOROLOGICAL-SATELLITE (space-to-Earth)  MOBILE except aeronautical mobile  5.461A | | |
| 7 550-7 750 FIXED  FIXED-SATELLITE (space-to-Earth)  MOBILE except aeronautical mobile | | |

**Reasons:** No change in the band 7 375-7 750 MHz due to to incompatibility with existing services.

NOC INS/MLA/118A9A2/2

7 250-8 500 MHz

|  |  |  |
| --- | --- | --- |
| Allocation to services | | |
| Region 1 | Region 2 | Region 3 |
| 8 025-8 175 EARTH EXPLORATION-SATELLITE (space-to-Earth)  FIXED  FIXED-SATELLITE (Earth-to-space)  MOBILE 5.463  5.462A | | |
| 8 175-8 215 EARTH EXPLORATION-SATELLITE (space-to-Earth)  FIXED  FIXED-SATELLITE (Earth-to-space)  METEOROLOGICAL-SATELLITE (Earth-to-space)  MOBILE 5.463  5.462A | | |
| 8 215-8 400 EARTH EXPLORATION-SATELLITE (space-to-Earth)  FIXED  FIXED-SATELLITE (Earth-to-space)  MOBILE 5.463  5.462A | | |

**Reasons:** No change in the band 8 025-8 400 MHz due to to incompatibility with existing services.

SUP INS/MLA/118A9A2/3

RESOLUTION 758 (WRC‑12)

Allocation to the fixed-satellite service and the maritime-  
mobile satellite service in the 7/8 GHz range

**Reasons:** Further consideration and/or study are not needed any more.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_