|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15) Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Document 121-E** |
|  | **19 October 2015** |
|  | **Original: English** |
|  | |
| Benin (Republic of)/Burkina Faso/Côte d'Ivoire (Republic of)/ Gambia (Republic of the)/Ghana/Guinea (Republic of)/Mali (Republic of)/ Niger (Republic of the)/Nigeria (Federal Republic of)/Senegal (Republic of)/ Sierra Leone/Togolese Republic | |
| Proposals for the work of the conference | |
|  | |
| Agenda item 1.2 | |

1.2 to examine the results of ITU‑R studies, in accordance with Resolution **232 (WRC‑12)**, on the use of the frequency band 694-790 MHz by the mobile, except aeronautical mobile, service in Region 1 and take the appropriate measures;

Proposals

BEN/BFA/CTI/GMB/GHA/GUI/MLI/NGR/NIG/SEN/SRL/TGO/121/1

Issue D: Solutions for accommodating applications ancillary to broadcasting requirements

Method D2

Modification of the existing upper limits of frequency bands mentioned in RR No. **5.296** for the secondary allocation to 694 MHz and extension of that use to the applications ancillary to programme-making.

In order to accommodate the operability of the frequency band 694-790 MHz for applications ancillary to broadcasting and programme-making, a WRC Resolution needs to address the issue taking into account the process described in Resolution ITU-R 59.

For Method D2

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

MOD BEN/BFA/CTI/GMB/GHA/GUI/MLI/NGR/NIG/SEN/SRL/TGO/121/2

5.296 *Additional allocation:* in Albania, Germany, Saudi Arabia, Austria, Bahrain, Belgium, Benin, Bosnia and Herzegovina, Burkina Faso, Cameroon, Congo (Rep. of the), Côte d'Ivoire, Croatia, Denmark, Djibouti, Egypt, United Arab Emirates, Spain, Estonia, Finland, France, Gabon, Ghana, Iraq, Ireland, Iceland, Israel, Italy, Jordan, Kuwait, Latvia, The Former Yugoslav Republic of Macedonia, Libya, Liechtenstein, Lithuania, Luxembourg, Mali, Malta, Morocco, Moldova, Monaco, Niger, Norway, Oman, the Netherlands, Poland, Portugal, Qatar, the Syrian Arab Republic, Slovakia, the Czech Republic, the United Kingdom, Sudan, Sweden, Switzerland, Swaziland, Chad, Togo, Tunisia and Turkey, Angola, Botswana, Lesotho, Malawi, Mauritius, Mozambique, Namibia, Nigeria, South Africa, Tanzania, Zambia and Zimbabwe, the band 470-694 MHz is also allocated on a secondary basis to the land mobile service, intended for applications ancillary to broadcasting and programme-making. Stations of the land mobile service in the countries listed in this footnote shall not cause harmful interference to existing or planned stations operating in accordance with the Table in countries other than those listed in this footnote.     (WRC‑15)

*NOTE FOR SECRETARIAT − The countries names should be rearranged alphabetically at WRC‑15.*

*NOTE − Depending on the outcome of WRC-15, i.e., if this Method D2 is adopted by WRC-15, only one of the options below (modification of Resolution* ***232*** *or addition of two considerings in a new WRC-15 Resolution) should to be retained.*

MOD BEN/BFA/CTI/GMB/GHA/GUI/MLI/NGR/NIG/SEN/SRL/TGO/121/3

RESOLUTION 232 (rev.WRC‑15)

Use of the frequency band 694-790 MHz by the mobile, except aeronautical mobile, service in Region 1

The World Radiocommunication Conference (Geneva,2015)

considering

...

*aaa)* that in Region 1, a number of countries have deployments of applications ancillary to broadcasting and programme-making operating on a secondary basis, which provide tools for the daily content production for the broadcast service;

*bbb)* that further harmonization of spectrum for applications ancillary to broadcasting andprogramme-makingin the frequency band 694-790 MHz is subject to ITU‑R studies regarding possible solutions for global/regional harmonization of frequency bands and tuning ranges for electronic news gathering (ENG) use in accordance to Resolution ITU‑R 59;

or

ADD BEN/BFA/CTI/GMB/GHA/GUI/MLI/NGR/NIG/SEN/SRL/TGO/121/4

Draft New RESOLUTION [121-A12-Method-D2] (WRC-15)

The World Radiocommunication Conference (Geneva, 2015),

...

considering

...

*aaa)* that in Region 1, a number of countries have deployments of applications ancillary to broadcasting and programme-making operating on a secondary basis, which provide tools for the daily content production for the broadcast service;

*bbb)* that further harmonization of spectrum for applications ancillary to broadcasting and programme-making in the frequency band 694-790 MHz is subject to ITU‑R studies regarding possible solutions for global/regional harmonization of frequency bands and tuning ranges for electronic new gathering (ENG) use as in accordance to Resolution ITU‑R 59;

…

\_\_\_\_\_\_\_\_\_\_\_\_\_\_