|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19) Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 14 to Document 24-E** |
|  | **23 September 2019** |
|  | **Original: English** |
|  | |
| Asia-Pacific Telecommunity Common Proposals | |
| PROPOSALS FOR THE WORK OF THE CONFERENCE | |
|  | |
| Agenda item 1.14 | |

1.14 to consider, on the basis of ITU-R studies in accordance with Resolution **160 (WRC‑15)**, appropriate regulatory actions for high-altitude platform stations (HAPS), within existing fixed-service allocations;

Introduction

APT Members support no changes to the Radio Regulations (Method A as contained in the CPM Report) to ensure protection of all existing services to which frequency bands are allocated and their future development in the frequency bands 6 440-6 520 MHz and 6 560-6 640 MHz.

In addition, APT Members are of the view that any consideration of the frequency band 24.25-27.5 GHz in Region 2 under this agenda item should not limit the possibility to identify the band for IMT on a global basis under WRC-19 agenda item 1.13.

APT Members consider that protection of all existing services to which frequency bands are allocated and their future development should be ensured.

No consensus was reached among APT Members on any Method to address this agenda item in the frequency bands 27.9-28.2 GHz, 31-31.3 GHz, 38-39.5 GHz, 47.2-47.5 GHz and 47.9-48.2 GHz.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

NOC ACP/24A14/1

5 570-6 700 MHz

|  |  |  |
| --- | --- | --- |
| Allocation to services | | |
| Region 1 | Region 2 | Region 3 |
|  |  |  |
| 5 925-6 700 FIXED 5.457  FIXED-SATELLITE (Earth-to-space) 5.457A 5.457B  MOBILE 5.457C  5.149 5.440 5.458 | | |

**Reasons:** No changes are supported in the bands 6 440-6 520 MHz and 6 560-6 640 MHz.

NOC ACP/24A14/2

RESOLUTION 150 (WRC‑12)

Use of the bands 6 440-6 520 MHz and 6 560-6 640 MHz by gateway links   
for high-altitude platform stations in the fixed service

**Reasons:** No changes are supported in the bands 6 440-6 520 MHz and 6 560-6 640 MHz.

SUP ACP/24A14/3#50365

RESOLUTION 160 (WRC‑15)

Facilitating access to broadband applications delivered   
by high-altitude platform stations

**Reasons:** Further work is not required.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_