|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 20 toDocument 36-E** |
|  | **2 October 2019** |
|  | **Original: Russian** |
|  |
| Uzbekistan (Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 8 |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC-07)**;

Introduction

In accordance with Resolution **26** (**Rev**.**WRC-07**), the Administration of Uzbekistan has examined the footnotes to the Table of Frequency Allocations and proposes that the country name of Uzbekistan be deleted from the footnotes contained in annex hereto.

Proposal

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD UZB/36A20/1

3 230-5 003 kHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 4 438-4 488FIXEDMOBILE except aeronautical mobile (R)Radiolocation 5.132A | 4 438-4 488FIXEDMOBILE except aeronautical mobile (R)RADIOLOCATION 5.132A | 4 438-4 488FIXEDMOBILE except aeronautical mobileRadiolocation 5.132A |
| MOD 5.132B |  |  |

MOD UZB/36A20/2

5.132B *Alternative allocation:*in Armenia, Belarus, Moldova and Kyrgyzstan, the frequency band 4 438-4 488 kHz is allocated to the fixed and mobile, except aeronautical mobile (R), services on a primary basis.     (WRC‑19)

**Reasons:** The reference to Uzbekistan in footnote No. **5.132B** of the Radio Regulations (RR) is no longer required.

MOD UZB/36A20/3

5 003-7 000 kHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 5 250-5 275FIXEDMOBILE except aeronautical mobileRadiolocation 5.132A | 5 250-5 275FIXEDMOBILE except aeronautical mobileRADIOLOCATION 5.132A | 5 250-5 275FIXEDMOBILE except aeronautical mobileRadiolocation 5.132A |
| MOD 5.133A |  |  |

MOD UZB/36A20/4

5.133A *Alternative allocation:*  in Armenia, Belarus, Moldova and Kyrgyzstan, the frequency bands 5 250-5 275 kHz and 26 200-26 350 kHz are allocated to the fixed and mobile, except aeronautical mobile, services on a primary basis.     (WRC‑19)

**Reasons:** The reference to Uzbekistan in footnote RR No. **5.133A** is no longer required.

MOD UZB/36A20/5

7 450-13 360 kHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 9 040-9 305FIXED | 9 040-9 400FIXED | 9 040-9 305FIXED |
| 9 305-9 355FIXEDRadiolocation 5.145A | 9 305-9 355FIXEDRadiolocation 5.145A |
| MOD 5.145B |  |
| 9 355-9 400FIXED | 9 355-9 400FIXED |

MOD UZB/36A20/6

5.145B *Alternative allocation:*in Armenia, Belarus, Moldova and Kyrgyzstan, the frequency bands 9 305-9 355 kHz and 16 100-16 200 kHz are allocated to the fixed service on a primary basis.     (WRC‑19)

**Reasons:** The reference to Uzbekistan in footnote RR No. **5.145B** is no longer required.

MOD UZB/36A20/7

13 360-18 030 kHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 13 450-13 550FIXEDMobile except aeronautical mobile (R)Radiolocation 5.132A | 13 450-13 550 FIXED Mobile except aeronautical mobile (R) Radiolocation 5.132A |
| MOD 5.149A |  |
| 16 100-16 200FIXEDRadiolocation 5.145A | 16 100-16 200FIXEDRADIOLOCATION 5.145A | 16 100-16 200FIXEDRadiolocation 5.145A |
| MOD 5.145B |  |  |

MOD UZB/36A20/8

5.149A *Alternative allocation:*  in Armenia, Belarus, Moldova and Kyrgyzstan, the frequency band 13 450-13 550 kHz is allocated to the fixed service on a primary basis and to the mobile, except aeronautical mobile (R), service on a secondary basis.     (WRC‑19)

**Reasons:** The reference to Uzbekistan in footnote RR No. **5.149A** is no longer required.

MOD UZB/36A20/9

23 350-27 500 kHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 24 450-24 600FIXEDLAND MOBILERadiolocation 5.132A | 24 450-24 650FIXEDLAND MOBILERADIOLOCATION 5.132A | 24 450-24 600FIXEDLAND MOBILERadiolocation 5.132A |
| MOD 5.158 |  |
| 26 200-26 350FIXEDMOBILE except aeronautical mobileRadiolocation 5.132A | 26 200-26 420FIXEDMOBILE except aeronautical mobileRADIOLOCATION 5.132A | 26 200-26 350FIXEDMOBILE except aeronautical mobileRadiolocation 5.132A |
| MOD 5.133A |  |

MOD UZB/36A20/10

5.158 *Alternative allocation:*  in Armenia, Belarus, Moldova and Kyrgyzstan, the frequency band 24 450-24 600 kHz is allocated to the fixed and land mobile services on a primary basis.     (WRC‑19)

**Reasons:** The reference to Uzbekistan in footnote RR No. **5.158** is no longer required.

MOD UZB/36A20/11

27.5-40.98 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 38.25-39FIXEDMOBILE | 38.25-39.986FIXEDMOBILE | 38.25-39.5FIXEDMOBILE |
| 39-39.5FIXEDMOBILERadiolocation 5.132AMOD 5.159 |  |  |
| 39.5-39.986FIXEDMOBILE |  | 39.5-39.986FIXEDMOBILERADIOLOCATION 5.132A |

MOD UZB/36A20/12

5.159 *Alternative allocation:*  in Armenia, Belarus, Moldova and Kyrgyzstan, the frequency band 39‑39.5 MHz is allocated to the fixed and mobile services on a primary basis.     (WRC‑19)

**Reasons:** The reference to Uzbekistan in footnote RR No. **5.159** is no longer required.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_