|  |  |  |  |
| --- | --- | --- | --- |
| A close up of a sign  Description automatically generated | **World Radiocommunication Conference (WRC-23) Dubai, 20 November - 15 December 2023** | |  |
|  | |  | |
|  | |  | |
| PLENARY MEETING | | **Addendum 1 to Document 65(Add.2)-E** | |
|  | | **29 September 2023** | |
|  | | **Original: English** | |
|  | | | |
| European Common Proposals | | | |
| Proposals for the work of the conference | | | |
|  | | | |
| Agenda item 1.2 | | | |

1.2 to consider identification of the frequency bands 3 300-3 400 MHz, 3 600‑3 800 MHz, 6 425-7 025 MHz, 7 025-7 125 MHz and 10.0-10.5 GHz for International Mobile Telecommunications (IMT), including possible additional allocations to the mobile service on a primary basis, in accordance with Resolution **245 (WRC‑19)**;

**Part 1 – Frequency band 3 300-3 400 MHz in Region 1**

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

NOC EUR/65A2A1/1

5.429A *Additional allocation*:  in Angola, Benin, Botswana, Burkina Faso, Burundi, Djibouti, Eswatini, Ghana, Guinea, Guinea-Bissau, Lesotho, Liberia, Malawi, Mauritania, Mozambique, Namibia, Niger, Nigeria, Rwanda, Sudan, South Sudan, South Africa, Tanzania, Chad, Togo, Zambia and Zimbabwe, the frequency band 3 300‑3 400 MHz is allocated to the mobile, except aeronautical mobile, service on a primary basis. Stations in the mobile service operating in the frequency band 3 300-3 400 MHz shall not cause harmful interference to, or claim protection from, stations operating in the radiolocation service.     (WRC‑19)

NOC EUR/65A2A1/2

5.429B In the following countries of Region 1 south of 30° parallel north: Angola, Benin, Botswana, Burkina Faso, Burundi, Cameroon, Congo (Rep. of the), Côte d’Ivoire, Egypt, Eswatini, Ghana, Guinea, Guinea-Bissau, Kenya, Lesotho, Liberia, Malawi, Mauritania, Mozambique, Namibia, Niger, Nigeria, Uganda, the Dem. Rep. of the Congo, Rwanda, Sudan, South Sudan, South Africa, Tanzania, Chad, Togo, Zambia and Zimbabwe, the frequency band 3 300-3 400 MHz is identified for the implementation of International Mobile Telecommunications (IMT). The use of this frequency band shall be in accordance with Resolution **223 (Rev.WRC‑19)**. The use of the frequency band 3 300-3 400 MHz by IMT stations in the mobile service shall not cause harmful interference to, or claim protection from, systems in the radiolocation service, and administrations wishing to implement IMT shall obtain the agreement of neighbouring countries to protect operations within the radiolocation service. This identification does not preclude the use of this frequency band by any application of the services to which it is allocated and does not establish priority in the Radio Regulations.     (WRC‑19)

**Reasons:** CEPT does not support amendments to RR Nos. **5.429A** and **5.429B** which could extend them to countries north of 30° parallel north. Thus, CEPT does not support an IMT identification for the entire Region 1. Furthermore, CEPT opposes amending the footnote to change the regulatory provisions applicable to IMT stations in the band. In particular, IMT stations shall not cause harmful interference to, or claim protection from, systems in the radiolocation service in various national and international operational environments and shall meet unwanted emission levels specified in the relevant ITU-R Recommendations. In addition, protection of FSS in the frequency band 3 400-3 800 MHz should also be ensured, as appropriate.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_