|  |  |  |
| --- | --- | --- |
| A close up of a sign  Description automatically generated | **World Radiocommunication Conference (WRC-23)Dubai, 20 November - 15 December 2023** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Document 69-E** |
|  | **6 October 2023** |
|  | **Original: English** |
|  |
| South Sudan (Republic of) |
| Proposals for the work of the Conference |
|  |
| Agenda item 1.1 |

1.1 to consider, based on the results of ITU‑R studies, possible measures to address, in the frequency band 4 800-4 990 MHz, protection of stations of the aeronautical and maritime mobile services located in international airspace and waters from other stations located within national territories, and to review the power flux-density criteria in No. **5.441B** in accordance with Resolution **223 (Rev.WRC‑19)**;

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD SSD/69/1

5.441B In Angola, Armenia, Azerbaijan, Benin, Botswana, Brazil, Burkina Faso, Burundi, Cambodia, Cameroon, China, Côte d’Ivoire, Djibouti, Eswatini, Russian Federation, Gambia, Guinea, Iran (Islamic Republic of), Kazakhstan, Kenya, Lao P.D.R., Lesotho, Liberia, Malawi, Mauritius, Mongolia, Mozambique, Nigeria, Uganda, Uzbekistan, the Dem. Rep. of the Congo, Kyrgyzstan, the Dem. People's Rep. of Korea, Sudan, South Sudan, South Africa, Tanzania, Togo, Viet Nam, Zambia and Zimbabwe, the frequency band 4 800-4 990 MHz, or portions thereof, is identified for use by administrations wishing to implement International Mobile Telecommunications (IMT). This identification does not preclude the use of this frequency band by any application of the services to which it is allocated and does not establish priority in the Radio Regulations. The use of IMT stations is subject to agreement obtained under No. **9.21** with concerned administrations, and IMT stations shall not claim protection from stations of other applications of the mobile service. In addition, before an administration brings into use an IMT station in the mobile service, it shall ensure that the power flux-density (pfd) produced by this station does not exceed −155 dB(W/(m2 · 1 MHz)) produced up to 19 km above sea level at 20 km from the coast, defined as the low-water mark, as officially recognized by the coastal State. This pfd criterion is subject to review at WRC‑23. Resolution **223 (Rev.WRC‑19)** applies. This identification shall be effective after WRC‑19.     (WRC‑23)

**Reasons:** South Sudan wants to identify the frequency band 4 800-4 990 MHz, or portions thereof, for the implementation of International Mobile Telecommunications (IMT).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_