|  |
| --- |
| **Report ITU-R BT.2469-2**  **(11/2021)** |
| **Typical frequency sharing characteristics for digital terrestrial broadcasting systems in the frequency band 174-230 MHz** |
| **BT Series**  **Broadcasting service**  **(television)** |

Foreword

The role of the Radiocommunication Sector is to ensure the rational, equitable, efficient and economical use of the radio-frequency spectrum by all radiocommunication services, including satellite services, and carry out studies without limit of frequency range on the basis of which Recommendations are adopted.

The regulatory and policy functions of the Radiocommunication Sector are performed by World and Regional Radiocommunication Conferences and Radiocommunication Assemblies supported by Study Groups.

# Policy on Intellectual Property Right (IPR)

ITU-R policy on IPR is described in the Common Patent Policy for ITU-T/ITU-R/ISO/IEC referenced in Resolution ITU‑R 1. Forms to be used for the submission of patent statements and licensing declarations by patent holders are available from <http://www.itu.int/ITU-R/go/patents/en> where the Guidelines for Implementation of the Common Patent Policy for ITU‑T/ITU‑R/ISO/IEC and the ITU-R patent information database can also be found.

|  |  |
| --- | --- |
| Series of ITU-R Reports  (Also available online at <http://www.itu.int/publ/R-REP/en>) | |
| **Series** | Title |
| **BO** | Satellite delivery |
| **BR** | Recording for production, archival and play-out; film for television |
| **BS** | Broadcasting service (sound) |
| **BT** | Broadcasting service (television) |
| **F** | Fixed service |
| **M** | Mobile, radiodetermination, amateur and related satellite services |
| **P** | Radiowave propagation |
| **RA** | Radio astronomy |
| **RS** | Remote sensing systems |
| **S** | Fixed-satellite service |
| **SA** | Space applications and meteorology |
| **SF** | Frequency sharing and coordination between fixed-satellite and fixed service systems |
| **SM** | Spectrum management |

|  |
| --- |
|  |

|  |
| --- |
| ***Note****: This ITU-R Report was approved in English by the Study Group under the procedure detailed in Resolution ITU-R 1.* |

*Electronic Publication*

Geneva, 2021

© ITU 2021

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without written permission of ITU.

REPORT ITU-R BT.2469-2

Typical frequency sharing characteristics for digital terrestrial broadcasting systems in the frequency band 174-230 MHz

(2019-03/2021-11/2021)

TABLE OF CONTENTS

***Page***

[Policy on Intellectual Property Right (IPR) ii](#_Toc88812618)

[1 Introduction 3](#_Toc88812619)

[2 Broadcasting description 3](#_Toc88812620)

[2.1 Broadcasting protection criteria 3](#_Toc88812621)

[2.2 Broadcast service requirements 3](#_Toc88812622)

[2.3 Assessment of interference impact on the broadcast coverage 4](#_Toc88812623)

[2.4 Propagation considerations for interference assessments 6](#_Toc88812624)

[2.5 Aggregation of interference 6](#_Toc88812625)

[2.6 Comparative evaluations 6](#_Toc88812626)

[2.7 Inclusion of noise in interference assessments 6](#_Toc88812627)

[3 Television Systems 7](#_Toc88812628)

[3.1 Television transmission parameters for use in sharing and compatibility studies 7](#_Toc88812629)

[3.2 Television reception parameters for use in sharing and compatibility studies 12](#_Toc88812630)

[4 Sound systems 26](#_Toc88812631)

[4.1 Sound transmission parameters for use in sharing and compatibility studies 26](#_Toc88812632)

[4.2 Sound reception parameters for use in sharing and compatibility studies 28](#_Toc88812633)

[Annex 1 List of relevant ITU-R Reports and Recommendations 33](#_Toc88812634)

[Annex 2 General definitions 35](#_Toc88812635)

[A2.1 Broadcasting coverage area and service area planning 35](#_Toc88812636)

[A2.2 Definition of reception location probability 35](#_Toc88812637)

[Annex 3 Allotment reference networks 35](#_Toc88812638)

[A3.1 DTT Single frequency networks (Allotments)(GE06) 35](#_Toc88812639)

[A3.2 DSB Single frequency networks (Allotments)(GE06) 39](#_Toc88812640)

[Annex 4 Calculation of minimum field strength and minimum median equivalent field strength 41](#_Toc88812641)

[Annex 5 DTTB Link budgets 42](#_Toc88812642)

[A5.1 DVB-T 42](#_Toc88812643)

[A5.2 DVB-T2 45](#_Toc88812644)

[A5.3 ATSC 48](#_Toc88812645)

[A5.4 ISDB-T 50](#_Toc88812646)

[A5.5 DTMB 51](#_Toc88812647)

[Annex 6 DSB link budgets 53](#_Toc88812648)

[A6.1 DAB 53](#_Toc88812649)

# 1 Introduction

This Report contains a summary of the reference frequency sharing characteristics of Band III (174‑230 MHz) digital terrestrial broadcasting (DTB) systems, television and sound, required for relevant compatibility studies[[1]](#footnote-1).

Quotes from existing text in ITU-R are highlighted through the use of *Italics*.

It should be noted that for Band I, II, III, IV and V systems broadcasters quote antenna gains and effective radiated power (ERP) relative to a dipole. So, for example, a DTT receiving antenna with a quoted gain of 7 dB has a gain of 9.15 dBi when referenced to an isotropic source. Also, a broadcast station with a quoted ERP of 20 kW (43 dBW) has an e.i.r.p. of 75.15 dBm.

# 2 Broadcasting description

## 2.1 Broadcasting protection criteria

Broadcasting protection criteria are based on local interference considerations such as reception location probability, degradation to reception location probability in the presence of additional interference, *I*/*N* limitation and degradation to *C*/*N*.

Details about the protection requirements for the broadcasting service can be found in particular in Recommendation [ITU-R BT/BS.1895](http://www.itu.int/rec/R-REC-BT.1895/en) – Protection criteria for terrestrial broadcasting systems, and Report ITU-R BT.2265 – Guidelines for the assessment of interference into the broadcasting service. Further references are listed in Annex 1.

## 2.2 Broadcast service requirements

Terrestrial broadcasting services are required by many administrations to cover a high percentage of the population/households (e.g. 98%) or geographic regions (e.g. the entire country), in accordance with statutory requirements or commercial agreements. Reception in the area defined by this coverage requirement is stipulated for continuous use, for a specified time availability[[2]](#footnote-2), within the hours of transmission. This coverage requirement (as distinct from the coverage area of the broadcast transmission) applies within the service area that is licensed and protected.

Within the broadcast service area, interference effects can be assessed in many ways, but the overriding issue is how they may translate in terms of reducing the ability of the serving station or network to meet the coverage requirement of the broadcasting service. A reduction in the ability to meet the coverage requirement effectively translates to a loss of access to broadcast receiving stations for the specified time availability. Broadcast service planning methods are based on meeting a prescribed coverage requirement.

In cases where interference is from a distant source(s) outside the service area – typically, because of the distance such interference is co-channel – interference can usually be assessed in terms of limits on *I*/*N* only.

In cases where interference is from a source or sources within the service area – typically, because of the distance, adjacent-channel interference – interference can be initially assessed in terms of limits on *I*/*N*. However, in this case when calculating *I*/*N* a minimum distance, between the interferer and victim receiver, needs to be specified, which could be, for example - the distance associated with the minimum coupling loss.

Where further analysis is required, the impact to coverage of interference is normally assessed in terms of reception location probability. In such cases a judgement has to be made as to the acceptable reduction in area or population that, as a result of interference, can no longer receive a service for the specified time. What constitutes an acceptable reduction in service will depend on the statutory requirements and commercial agreements applicable to the affected service.

Specifically, the broadcast service delivery to the target population within the broadcast service area has been based on the expectation of a signal quality with minimum interruption[[3]](#footnote-3).

## 2.3 Assessment of interference impact on the broadcast coverage

### 2.3.1 Introduction

To assess the impact of interference into broadcast networks, it is necessary to apply the broadcast planning criteria with the new level of interference and compare the relative change in quality of service requirement before and after the introduction of the new source of interference. The issues that arise from the combination of this process and sharing studies are highlighted in § 2.3.2.

### 2.3.2 Standard broadcast planning practice

Planning of a digital terrestrial broadcasting service is based on specified parameters and requirements and providing a service that is quasi-error-free (QEF). These elements form the basis for the protection of the existing digital terrestrial broadcast networks.

A QEF condition of a digital television broadcasting signal means less than one uncorrected error event per hour and a corresponding BER can be calculated for an assumed transmission bit rate. For example, for a DTTB transmission with a bit rate of about 28 Mbit/s, QEF corresponds to BER less than 10−11 after the whole error correction process.

Which in the case of:

– DVB-T, ATSC1.0 and ISDB-T, this corresponds to BER less than 2 × 10−4 after Viterbi decoder or BER less than 10−11 after Reed-Solomon decoder.

– DVB-T2, DTMB and DTMB-A, this corresponds to BER less than 10−7 before BCH decoder or BER less than 10−11 after BCH decoder.

Any study of interference into a DTTB system must take account of QEF and the hour time window. Information on the use of Monte Carlo simulation to model interference to DTTB and application of a time window can be found in Report ITU-R BT. 2470[[4]](#footnote-4) and Recommendation BT.2136[[5]](#footnote-5).

For planning terrestrial broadcasting services, it is important to take into consideration the different elements of interference and the implications of temporal variations to separately identify when interference into the broadcast service arises from protection ratio failure and blocking due to overloading.

Spectrum planners are aware that a relaxation in the value or exclusion of certain interference assessment factors would reduce the ability to meet the broadcast coverage quality requirement. A relaxation of more than one of these parameters could result in a significant cumulative reduction in the extent to which a service area can be covered.

In the simple conceptual example below of planning the broadcasting service, it is assumed that the area covered by the broadcast transmission is circular and that up to four of the above interference assessment factors have been relaxed. Each reduction in the level of protection afforded by one of the broadcast interference assessment factors is represented by a ring identifying the potential percentage of the existing population or country that can no longer be reached under the broadcast coverage requirement, because of interference arising from the relaxation in the interference assessment factor(s).

A simplification of the spectrum planning process[[6]](#footnote-6) is provided for illustrative purposes in the diagram below. A service area with an existing broadcast provision that has been planned in accordance with the broadcast planning criteria and meets or exceeds the prescribed coverage requirement is represented in Fig. 1A by the dotted circle. That part of the service area in Fig. 1A, where the planned broadcast coverage has been reduced or lost due to the level of the interfering signal arising from the relaxation in one of the interference assessment factor(s) is shown in Fig. 1B.

In Fig. 1C the relaxation of multiple (in this case 4) interference assessment factors is aggregated to show the consequential impact on the planned broadcast service area, with the dotted area the only part of the planned broadcast service area in Fig. 1A, that remains covered by the planned broadcast transmission parameters. Not only is the effective broadcast service area significantly reduced but the target population within the planned service area is no longer served.

|  |  |  |
| --- | --- | --- |
| FIGURE 1A | FIGURE 1B | FIGURE 1C |
| Original area covered | Reduction in area covered  (relaxation of one factor) | Resulting area covered  (relaxation of four factors) |
|  |  |  |

In practice a broadcast service area is unlikely to be circular and the population lost to broadcast coverage will not be located in convenient rings around the edge of that service area. Both areas will be influenced by topographical factors, population distribution and the respective locations of the wanted and interfering transmitters.

Transmissions in adjacent bands /channels may also cause interference. Recommendations [ITU‑R BT.1368](http://www.itu.int/rec/R-REC-BT.1368/en), [ITU-R BT.2033](http://www.itu.int/rec/R-REC-BT.2033/en) and ITU-R BS.1660 as well as Reports [ITU-R BT.2215](http://www.itu.int/pub/R-REP-BT.2215) and [ITU‑R BT.2248](http://www.itu.int/pub/R-REP-BT.2248) contain additional information on this case.

## 2.4 Propagation considerations for interference assessments

Broadcast planning is based on the service being subject to occasional very limited outages during the year. Indeed, many administrations have followed this and other principles established in the [DTTB Handbook – Digital terrestrial television broadcasting in the VHF/UHF bands](file:///C:/Users/rbunch/AppData/Local/Microsoft/Windows/Temporary%20Internet%20Files/Content.Outlook/6RY171VC/%09%09%09%20%20%20%20%09%09publications.aspx?lang=en&parent=R-HDB-39) – and the [DSB Handbook – Terrestrial and satellite digital sound broadcasting to vehicular, portable and fixed receivers in the VHF/UHF bands](https://www.itu.int/en/publications/ITU-R/pages/publications.aspx?parent=R-HDB-20-2002&media=electronic) – in achieving global harmonization of terrestrial television and sound broadcasting systems. The protection criteria established in Recommendations ITU-R BT.1368 and ITU-R BT.2033 for protecting DTTB services and in ITU-R BS.1660 for DSB have been developed on the assumption that Recommendation [ITU-R P.1546](http://www.itu.int/rec/R-REC-P.1546/en) is used in interference assessment and it is essential to take this into consideration. It should be noted that Recommendation ITU‑R P.1546 has been the recommended propagation model for terrestrial television broadcast planning for over a decade. Application of a different propagation model for DTTB and DSB coverage/interference assessment may not necessarily be compatible with the planning criteria and protection ratios applied by administrations towards maintaining the required quality of coverage.

Administrations which currently have planned digital terrestrial broadcasting services are aware that, like several other radio communication services, interference assessment is based on an interfering signal exceeding an annual 1% of time limit based upon a methodology that includes Recommendation ITU-R P.1546.

## 2.5 Aggregation of interference

Appendix 3 to Annex 2 to Report [ITU-R BT.2265-2](http://www.itu.int/pub/R-REP-BT.2265) describes the methods for the aggregation of short-term interfering signals.

*Two methods for the computation of aggregate interference from multiple transmitters where individual path losses are temporally variable are recommended.*

*The first approach (“general method”) is based on a rigorous mathematical treatment of the joint variability of multiple paths, and can be used to estimate the aggregate received power at any percentage-time. The method uses Monte Carlo simulation involving multiple calculations for each path of interest, and would be appropriate for use in a situation where numerically-intensive computer simulation is already envisaged.*

*Recognizing that this approach may not always be appropriate (e.g. where a quick estimate is required without an iterative computer simulation), a simple alternative is also proposed (“simple method”). This method is currently only defined for the case where the aggregate power is to be estimated at 1% time, although it could be readily extended for use at other percentage-times.*

## 2.6 Comparative evaluations

When calculations are carried out with certain reference parameters and comparison calculations are to be carried out, the relevant reference parameters must be the same. For example, if single-entry field strength values are calculated at a 10 m DTB receive antenna height, then comparison multiple-entry field values should also be calculated at the same 10 m DTB receive antenna height.

## 2.7 Inclusion of noise in interference assessments

An important factor in terrestrial broadcast service planning is the need to take into consideration an allowance for the noise environment in which the terrestrial broadcast service is to be planned – these are rural, urban and suburban. It should also be noted that broadcast services are planned based upon the calculation of *C*/*N* prior to the introduction and deployment of other services which has the potential to increase the noise allowance calculation required in many environments.

A wanted broadcast signal must be sufficient to overcome noise for it to be receivable and in this respect thermal noise and noise figure are an essential part of any calculations. These are the fundamentals upon which the broadcast receivers deployed globally have been designed.

# 3 Television Systems

This section provides parameters for Band III television systems for use in sharing and compatibility studies. Section 3.1 provides transmission parameters, Section3.2 provides receiver parameters. Common parameters are provided at the start of each of these sections with sub-sections containing parameters specific to a given television technology, DVB-T/T2, ATSC, ISDB‑T, and DTMB.

## 3.1 Television transmission parameters for use in sharing and compatibility studies

### 3.1.0 Out of Band Masks

Information on DTTB transmitter spectrum masks to be used in compatibility studies is provided in Recommendation ITU-R BT.1206.

### 3.1.1 DTTB System B (DVB-T) reference broadcasting networks

Reference broadcast transmitter configurations are provided that are representative of actual deployments in the case of assignments. Information on the reference configurations used in the GE06 Agreement for allotment planning are provided in Annex 3.

#### 3.1.1.1 DVB-T and DVB-T2 Single transmitter case (assignments):

– High power

• ERP: 20 kW

• Effective antenna height: 300 m

• Antenna height a.g.l.: 100 m

• Antenna pattern:

○ Horizontal: Omnidirectional

○ Vertical antenna aperture: based on 12λ aperture with 2° beam tilt

– Medium power

• ERP: 2 kW

• Effective antenna height: 150 m

• Antenna height a.g.l.: 50 m

• Antenna pattern:

○ Horizontal: Omnidirectional

○ Vertical: based on 6λ aperture with 3.2° beam tilt

– Low power

• ERP: 250 W

• Effective antenna height: 50 m

• Antenna height a.g.l.: 20 m

• Antenna pattern:

○ Horizontal: Directional (cardioid)

○ Vertical: based on 4λ aperture with 6° beam tilt

The attenuation (Aϑ) of the horizontal radiation pattern with azimuth angle (ϑ) is given by:

dB

where:

where:


ϑ : azimuth angle

*k* : 0.4187 for 10 dB pattern minima.

The resulting pattern is shown in Fig. 2:

Figure 2

Low power DTT



Unlike high and medium power antennas which are usually omnidirectional, few low power DTT antenna are omnidirectional. Low power DTT antennas typically have a directional horizontal radiation pattern usually of a type cardioid (dipoles mounted on a pole) or consisting of one or more panel, Yagi or log-periodic elements. These antennas typically have minima in the HRP that are 10 dB or more below the maximum and may have lobes that occur at various azimuth angles, lobes typically being aligned with the desired service area.

As patterns of low power antenna vary considerably modelling all combinations of pattern in generic compatibility studies is usually not practical. Therefore, to better represent the horizontal radiation pattern of low power DTT it is proposed to base the generic model on the pattern of a cardioid antenna with a 10 dB minimum. Depending on the compatibility study being undertaken the orientation of the pattern (angle of azimuth) can be varied as required.

#### 3.1.1.2 Vertical radiation patterns

The normalized field strength in the vicinity of the broadcast transmitting station is a function of the vertical radiation pattern of the transmitting antenna. The equation below is an approximation to be used for sharing studies.



where:



and

*A* = the antenna vertical aperture in wavelengths

β = the beam tilt radians below the horizontal.

To allow for null fill the value of *E*(θ)should not go below the value shown in Table 1.

TABLE 1

Null fill values to be applied to vertical radiation patterns

|  |  |
| --- | --- |
|  | Limit on *E*(θ) |
| First null | 0.15 |
| Second null | 0.1 |

For the third null and at all angles of θbeyond the third null the value of *E*(θ)should not fall below 0.05.

*E*(θ)given above are linear values, to convert them to reduction values in dB the following equation is used:

### 3.1.2 ATSC Reference broadcasting networks

Reference broadcast transmitter configurations are provided that are representative of actual deployments[[7]](#footnote-7).

#### 3.1.2.1 DTTB System A (ATSC) single transmitter

– High power

• e.r.p.: 160 kW

• Antenna height above average terrain (HAAT): 305 m

• Antenna pattern: Omnidirectional

– Medium power

• e.r.p.: 30 kW

• Antenna height above average terrain (HAAT): 610 m

• Antenna pattern: Omnidirectional

– Low power

• e.r.p.: 10 kW

• Antenna height above average terrain (HAAT): 1 000 m

• Antenna pattern: Omnidirectional

NOTE – The values provided are based on the premise that a higher antenna can cover a specific area with less power. The point being to avoid interference from transmitters operating in adjacent areas.

The specific numbers represent three typical scenarios frequently found in the United States of America and were derived from the FCC database. FCC rules (47CFR 73.614) describe the relationship between the maximum allowable ERP and HAAT.

#### 3.1.2.2 Vertical radiation pattern

The field strength in the vicinity of the broadcast VHF transmitting station is a function of the vertical radiation pattern of the transmitting antenna. The values in Table 2 below are to be used for sharing studies[[8]](#footnote-8).

TABLE 2

Vertical VHF radiation pattern

| Angle from horizon (degrees) | Relative field strength |
| --- | --- |
| 0.75 | 1.000 |
| 1.50 | 0.970 |
| 2.00 | 0.940 |
| 2.50 | 0.890 |
| 3.00 | 0.820 |
| 3.50 | 0.730 |
| 4.00 | 0.650 |
| 5.00 | 0.470 |
| 6.00 | 0.330 |
| 7.00 | 0.280 |
| 8.00 | 0.280 |
| 9.00 | 0.280 |
| 10.00 | 0.250 |

To allow for null fill the value of the relative field strength should not go below 0.250 at all angles.

*Relative Field Strength* given above are linear values, to convert them to reduction values in dB the following equations is used:

### 3.1.3 ISDB-T Reference broadcasting networks

Reference broadcast transmitter configurations are provided that are representative of actual deployments.

#### 3.1.3.1 DTTB System C (ISDB-T) single transmitter

– High power

• e.r.p.: 16 kW

• Antenna height above average terrain (HAAT): 150 m

• Antenna pattern: Omnidirectional

– Medium power

• e.r.p.: 1.6 kW

• Antenna height above average terrain (HAAT): 150 m

• Antenna pattern: Omnidirectional

– Low power

• e.r.p.: 0.16 kW

• Antenna height above average terrain (HAAT): 150 m

• Antenna pattern: Omnidirectional

#### 3.1.3.2 Vertical radiation pattern

The normalized field strength in the vicinity of the broadcast transmitting station is a function of the vertical radiation pattern of the transmitting antenna. The equation below is an approximation to be used for sharing studies.



where:



and

*A* = the antenna vertical aperture in wavelengths

β = the beam tilt radians below the horizontal.

*E*(θ)given above are linear values, to convert them to reduction values in dB the following equation is used:

### 3.1.4 DTMB Reference broadcasting networks

Reference broadcast transmitter configurations are provided that are representative of actual deployments.

#### 3.1.4.1 DTTB System D (DTMB) single transmitter

– High power

• ERP: 20kW

• Effective antenna height: 300 m

• Antenna height a.g.l.: 100 m

• Antenna pattern: Omnidirectional

– Medium power

• ERP: 2 kW

• Effective antenna height: 150 m

• Antenna height a.g.l.: 50 m

• Antenna pattern: Omnidirectional

– Low power

• ERP: 250 W

• Effective antenna height: 50 m

• Antenna height a.g.l.: 20 m

• Antenna pattern: Omnidirectional

#### 3.1.4.2 Vertical radiation pattern

The normalized field strength in the vicinity of the broadcast transmitting station is a function of the vertical radiation pattern of the transmitting antenna. The equation below is an approximation to be used for sharing studies.



where:



and

*A* = the antenna vertical aperture in wavelengths

β = the beam tilt radians below the horizontal.

*E*(θ)given above are linear values, to convert them to reduction values in dB the following equation is used:

## 3.2 Television reception parameters for use in sharing and compatibility studies

### 3.2.1 Parameters Common to all systems

#### 3.2.1.1 Fixed antenna reference height

The reference receiving antenna height considered to be representative in calculating the field strength for fixed reception is 10 m above ground level.

#### 3.2.1.2 Fixed antenna radiation pattern

Standard radiation patterns for receiving antennas for Bands I, III, IV and V are as shown in Fig. 3, which are given in Recommendation [ITU-R BT.419-3](http://www.itu.int/rec/R-REC-BT.419/en).

Figure 3



#### 3.2.1.3 Portable antenna reference height

For portable (indoor and outdoor) reception, a receiving antenna height of 1.5 m above ground level is used.

#### 3.2.1.4 Polarization discrimination for portable reception

Polarization discrimination should not be taken into account in frequency planning for portable reception[[9]](#footnote-9).

#### 3.2.1.5 Height loss correction

For portable (indoor and outdoor) reception, a receiving antenna height of 1.5 m above ground level is used. The same receiving antenna height is also used for mobile reception.

However, in broadcasting, it is common practice for fixed reception to calculate the field strength at 10 m, or at the height of the surrounding clutter if it is greater than 10m, for example in an urban environment[[10]](#footnote-10). In some cases a 10 m reference height is also used as the starting point in calculations for portable and mobile reception with an appropriate height loss taken into account to derive the required value at 1.5 m.

The height-loss values for portable and for mobile reception for reference frequencies are given in Table 3.

TABLE 3

Suburban and urban height loss in Bands III[[11]](#footnote-11)

|  |  |
| --- | --- |
| Frequency (MHz) | 200 |
| Suburban height loss (dB) (10 m terminal and clutter height to 1.5 m receiver height) | 12 |
| Urban height loss (dB) (20 m terminal and clutter height to 1.5 m receiver height) | 19 |

#### 3.2.1.6 Building entry loss

The methodology described in Recommendation ITU-R [P.2109](http://www.itu.int/rec/R-REC-P.2109/en) for calculating building loss should be used in sharing and compatibility studies involving broadcast systems.

Recommendation ITU-R [P.2109](http://www.itu.int/rec/R-REC-P.2109/en) covers a full range of building types of traditional and thermally efficient construction. For sharing and compatibility studies, involving broadcast systems, that use Recommendation ITU-R [P.2109](http://www.itu.int/rec/R-REC-P.2109/en), whenever a single representative value is required (for example, in an MCL analysis), the parameters provided in Table 4 should be used. This is independent of coverage planning. For dynamic or statistical analysis (for example, in a Monte Carlo simulation), the full distribution function of Recommendation ITU-R [P.2109](http://www.itu.int/rec/R-REC-P.2109/en) should be used.

TABLE 4

P.2109 Broadcast building entry loss parameters to use in sharing and compatibility studies

|  |  |  |
| --- | --- | --- |
| Building type | Environment | Probability building entry loss not exceeded |
| Traditional | Suburban | 50% |
| Traditional | Urban | 70% |

NOTE – Studies of building entry loss have meant figures have changed over time with the current version of Recommendation ITU-R [P.2109](http://www.itu.int/rec/R-REC-P.2109/en) representing the latest work. The parameters specified in Table 4 provide a building entry loss aligned with values derived using parameters supplied in older documents, for example Recommendation ITU-R P.1812-2 and the low building class in Recommendation ITU-R BT.2033-1.

#### 3.2.1.7 Antenna gain frequency correction

Within any frequency band, the variation of antenna gain with other frequency may be taken into account by the addition of a correction term:



where:

Corr : correction term

F*A* : actual working frequency being considered

F*R* : reference frequency.

Minimum median field strength levels for other frequencies are derived by interpolation as described in § 3.2.1.8.

#### 3.2.1.8 Interpolation of reference field strength values

For frequencies other than those quoted in tables, as described in Appendix 3.5 of Chapter 3 of the Final Acts of RRC06, the reference field-strength values should be adjusted by adding the correction factor defined according to the following rule:

– (*Emed*)*ref*(*f*) = (*Emed*)*ref*(*fr*) + Corr;

– for fixed reception, Corr = 20 log10 (*f/fr*), where *f* is the actual frequency and *fr* the reference frequency in the table;

– for portable reception and mobile reception, Corr = 30 log10 (*f/fr*) where *f* is the actual frequency and *fr* the reference frequency in the table.

#### 3.2.1.9 Location variability correction[[12]](#footnote-12)

Recommendation ITU‑R P.1546‑6, Annex 5 Table 2, gives a standard deviation of 5.5 dB for wideband broadcast signals. This value should be used to determine the field-strength variation at locations.

### 3.2.2 DVB-T / DVB-T2 – System specific receive parameters

#### 3.2.2.1 General parameters

TABLE 5

General DVB-T/T2 parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Fixed reception | Portable reception (outdoor/Mobile  or indoor) |
| DVB-T/T2 | DVB-T/T2 |
| Signal band width (MHz) | 6 6.66 | |
| Thermal noise density (kT0) (dBm/Hz) | −173.98 | |
| Receiver noise figure (1), (2) (dB) | 5 / 6 | |
| Allowance for manmade noise (3) (dB) | 2 | 8 |
| (1) ITU-R BT 1368-13, Table 53.  (2) ITU-R BT 2033-1, Table 12.  (3) ITU-R BT 2033-1, Table 31. | | |

#### 3.2.2.2 Carrier to noise

Within GE06, Recommendations ITU-R BT.1368-13 for DVB-T and in ITU-R BT.2033-1 for DVB‑T2, carrier to noise figures are provided. For compatibility and sharing studies the values in Table 6 should be used for both systems.

TABLE 6

Carrier-to-noise ratio DVB-T and DVB-T2

|  |  |
| --- | --- |
| Fixed reception | Portable reception |
| 20 dB | 18 dB |

#### 3.2.2.3 Fixed reception definition

Fixed reception is defined as reception where a directional receiving antenna mounted at roof level is used.

It is assumed that near-optimal reception conditions (within a relatively small volume on the roof) are found when the antenna is installed.

In calculating the field strength for fixed antenna reception, a receiving antenna height of 10 m above ground level is considered to be representative for the broadcasting service. Other heights might be used for other services.

##### 3.2.2.3.1 Fixed antenna system gain

For fixed reception the antenna gain values (relative to a half-wave dipole) used in the derivation of the minimum median equivalent field-strength values are given in Table 7.

TABLE 7

Antenna gain (relative to a half-wave dipole) in Bands III

|  |  |
| --- | --- |
| Frequency (MHz) | 200 |
| Antenna gain (dBd) (1) | 7 |
| Feeder loss (dB) | 2 |
| Antenna system gain (dBd) (2) | 5 |
| (1) Recommendation ITU-R BT.1368-13, Table 53 gives an antenna gain of 5 dBd with a feeder loss of 3 dB for a total antenna system gain of 2 dBd. GE06 and Recommendation ITU-R BT.2033-1 use an antenna gain of 7 dBd with a feeder loss of 2 dB for a total antenna system gain of 5 dBd.  (2) The antenna gain is equivalent to 9.15 dBi and the antenna system gain is equivalent to 7.15 dBi. | |

##### 3.2.2.3.2 Polarization discrimination fixed reception

For calculation of interference:

– For Terminal station (UE) polarization discrimination must not be applied.

– For Base Station (BS) polarization discrimination may be applied. The combined value of polarization discrimination and discrimination offered by receive aerial directivity must not be more than 12 dB[[13]](#footnote-13).

##### 3.2.2.3.3 Location probability – fixed reception

For fixed reception, the location probability as given in Table 8 should be used.

TABLE 8

Location probability for fixed reception

|  |  |
| --- | --- |
| System | DVB-T(GE06)/DVB-T2 |
| Location Probability (%) | 95 |

#### 3.2.2.4 Portable reception definition

Portable reception is defined as:

– outdoor – which means reception by a portable receiver with an attached or built-in antenna is used outdoors at no less than 1.5 m above ground level;

– indoor – which means reception by a portable receiver with an attached or built-in antenna is used indoors at no less than 1.5 m above floor level in rooms with a window in an external wall.

In both cases, it is assumed that optimal receiving conditions will be found by moving the antenna up to 0.5 m in any direction and extreme cases, such as reception in completely shielded rooms, are disregarded.

##### 3.2.2.4.1 Portable receive antenna gain

Recommendations ITU-R BT.1368-13 in its Annex 6, § 4.1 and ITU-R BT.2033-1 in Table 12 give information on antennas for portable reception. For portable reception, an omnidirectional antenna pattern should be applied with no feeder loss. For compatibility and sharing studies the antenna gain (relative to a half-wave dipole) given in Table 9 should be used for both systems.

TABLE 9

Antenna gain (dBd) for portable reception

|  |  |
| --- | --- |
| Band | Gain (dBd) |
| Band III | –2.15 |
| Note: This is equivalent to 0 dBi. | |

##### 3.2.2.4.2 Polarization discrimination portable reception

Polarization discrimination should not be taken into account in frequency planning for portable reception[[14]](#footnote-14).

##### 3.2.2.4.3 Location probability – portable reception

For portable reception, the location probability as given in Table 10 should be used.

TABLE 10

Location probability for portable reception

|  |  |
| --- | --- |
| System | DVB-T/DVB-T2(GE06) |
| Portable location probability (%) | 95 |

#### 3.2.2.5 Minimum field strength at 200 MHz

TABLE 11

DVB-T minimum field strength at 10 m a.g.l. suburban fr = 200 MHz

|  |  |  |
| --- | --- | --- |
| Fixed reception at 10 m for  95% location probability | Portable outdoor reception at 1.5 m for 95% location probability | Portable indoor reception at 1.5 m for 95% location probability |
| 46.4 dBµV/m | 69.5 dBµV/m | 87.2 dBµV/m |

TABLE 12

DVB-T2 minimum field strength at 10 m a.g.l. suburban fr = 200 MHz

|  |  |  |
| --- | --- | --- |
| Fixed reception at 10 m for  95% location probability | Portable outdoor reception at 1.5 m for 95% location probability | Portable indoor reception at 1.5 m for 95% location probability |
| 47.4 dBµV/m | 70.5 dBµV/m | 88.2 dBµV/m |

Minimum median field-strength levels for other frequencies than 200 MHz are derived by the correction described in § 3.2.1.8.

#### 3.2.2.6 Link budgets

Link budgets for DVB-T and DVB-T2 for fixed rooftop, portable outdoor and portable indoor reception are provided in Annex 5.

#### 3.2.2.7 Signal time percentage

TABLE 13

Time percentages used for sharing and compatibility studies

|  |  |  |
| --- | --- | --- |
| System | Wanted field strength | Interfering field strength |
| DVB-T/DVB-T2 | 50% | 1% |

#### 3.2.2.8 Protection ratios and overload threshold for interference from other services

Recommended values for protection ratios (PR) and overloading thresholdsfor DVB-T systems to be used in sharing studies can be found in Recommendation [ITU-R BT.1368-1](http://www.itu.int/pub/R-REP-BT.1368)3 Annex 2. Recommended values for protection ratios and overloading threshold for DVB-T2 receiverscan be found in Annex 1 of Recommendation ITU-R BT.2033-1.

#### 3.2.2.9 Correction of protection ratio figures for different ACLR values

Recommendation ITU-R BT.1368-13 Attachment 3 to Annex 2 describes calculation to derive protection ratios for all DTB systems for different ACLR values.

### 3.2.3 ATSC – System specific receive parameters

#### 3.2.3.1 General parameters

TABLE 14

General ATSC VHF parameters

|  |  |
| --- | --- |
| Parameter |  |
| Channel bandwidth (MHz) | 6 |
| Thermal noise density (kT0) (dBm/Hz) | –173.98 |
| Receiver noise figure (dB) | 10 |
| Man-made noise (dB) | 0 |

#### 3.2.3.2 Carrier to noise

TABLE 15

Carrier-to-noise ratio

|  |  |
| --- | --- |
| Fixed reception | Portable reception |
| 15.0 dB | 15.0 dB |

#### 3.2.3.3 Fixed antenna system gain

For fixed reception the antenna gain values (relative to a half-wave dipole) used in the derivation of the minimum median equivalent field-strength values are given in Table 16.

TABLE 16

Antenna gain (relative to a half-wave dipole) in Bands III

|  |  |
| --- | --- |
| Frequency (MHz) | 200 |
| Antenna gain (dBd) | 6 |
| Feeder loss (dB) | 2 |
| Antenna system gain (dBd) (1) | 4 |
| (1) Antenna system gain is equivalent 6.15 dBi. | |

#### 3.2.3.4 Polarization discrimination fixed reception

Polarization discrimination should not be taken into account in frequency planning for fixed reception due to the possibility of multipath interference.

#### 3.2.3.5 Location probability – fixed reception

For fixed reception, the location probability as given in Table 17 should be used.

TABLE 17

Location probability for fixed reception

|  |  |
| --- | --- |
| System | ATSC |
| Location probability (%) | 50 |

#### 3.2.3.6 Portable reception definition

Portable reception is defined as:

– outdoor – which means reception by a portable receiver with an attached or built-in antenna is used outdoors at no less than 1.5 m above ground level;

– indoor – which means reception by a portable receiver with an attached or built-in antenna is used indoors at no less than 1.5 m above floor level in rooms with a window in an external wall.

#### 3.2.3.7 Portable receive antenna gain

For portable reception Recommendation [ITU-R BT.1368-13](http://www.itu.int/rec/R-REC-BT.1368/en) gives in its Annex 6, § 4.1, information on antennas. For portable reception, an omnidirectional antenna should be applied. The antenna gain (relative to a half-wave dipole) is as given in Table 18.

TABLE 18

Antenna gain (dBd) for portable reception

|  |  |
| --- | --- |
| Band | Gain (dBd) |
| Band III | −2.15 (1) |
| (1) This is equivalent to 0 dBi. | |

#### 3.2.3.8 Portable reception definition

Polarization discrimination should not be taken into account in frequency planning for portable reception[[15]](#footnote-15).

#### 3.2.3.9 Location probability – portable reception

For portable indoor and outdoor reception, the location probability as given in Table 19 should be used.

TABLE 19

Location probability for portable reception

|  |  |
| --- | --- |
| System | ATSC |
| Location probability (%) | 50 |

#### 3.2.3.10 Minimum field strength at 200 MHz

TABLE 20

Minimum field strength at *fr* = 200 MHz

|  |  |
| --- | --- |
| Fixed reception at 10 m for  50% location probability | Portable outdoor reception at 1.5 m  for 50% location probability |
| 36 dBµV/m | 64.5 dBµV/m |

#### 3.2.3.11 Link budgets

Link budgets for ATSC for fixed rooftop and portable outdoor reception are provided in Annex 5.

#### 3.2.3.12 Signal time percentage

TABLE 21

Time percentages used for sharing and compatibility studies

|  |  |  |
| --- | --- | --- |
| System | Wanted field strength | Interfering field strength |
| ATSC | 90%[[16]](#footnote-16) | 1% |

#### 3.2.3.13 Protection ratios and overload threshold for interference from other services

Recommended values for protection ratios (PR) and overloading thresholdsfor ATSC systems to be used in sharing studies can be found in Annex 1 to Recommendation ITU-R BT.1368-13.

#### 3.2.3.14 Correction of protection ratio figures for different ACLR values

Recommendation ITU-R BT.1368-13 Attachment 3 to Annex 2 describes calculation to derive protection ratios for all DTTB systems for different ACLR values.

### 3.2.4 ISDB-T – System specific receive parameters

#### 3.2.4.1 General parameters

TABLE 22

ISDB-T VHF parameters

|  |  |
| --- | --- |
| Parameter |  |
| Signal band width (6 MHz system) (MHz) | 5.6 |
| Thermal noise density (kT0) (dBm/Hz) | −173.98 |
| Receiver noise figure (dB) | 5 |
| Allowance for manmade noise (dB) | 1 |

#### 3.2.4.2 Carrier to noise

TABLE 23

Carrier-to-noise ratio

|  |
| --- |
| Fixed reception |
| 20.1 dB |

#### 3.2.4.3 Fixed antenna system gain

For fixed reception the antenna gain values (relative to a half-wave dipole) used in the derivation of the minimum median equivalent field-strength values are given in Table 24.

TABLE 24

Antenna gain (relative to a half-wave dipole) in Bands III

|  |  |
| --- | --- |
| Frequency (MHz) | 200 |
| Antenna gain in relation to half-wave dipole (dBd) | 5 |
| Feeder loss (dB) | 3 |
| Antenna system gain (dBd) (1) | 2 |
| (1) Antenna system gain is equivalent to 4.15 dBi. | |

#### 3.2.4.4 Polarization discrimination fixed reception

Polarization discrimination should not be taken into account in frequency planning for fixed reception due to the possibility of multipath interference.

#### 3.2.4.5 Location probability – fixed reception

For fixed reception, the location probability as given in Table 25 should be used.

TABLE 25

Location probability for fixed reception

|  |  |
| --- | --- |
| System | ISDB-T |
| Location probability (%) | 95 |

#### 3.2.4.6 Minimum field strength at 200 MHz

TABLE 26

Minimum field strength at *fr* = 200 MHz

|  |
| --- |
| Fixed reception at 10 m  for 95% location probability |
| 47.6 dBµV/m |

Minimum median field-strength levels for other frequencies than 200 MHz are derived by the correction described in § 11.4, Report ITU-R BT.2383-1.

#### 3.2.4.7 Link budget – fixed outdoor reception

Link budgets for ISDB-T for fixed rooftop reception is provided in Annex 5.

#### 3.2.4.8 Signal time percentage

TABLE 27

Time percentages used for sharing and compatibility studies

|  |  |  |
| --- | --- | --- |
| System | Wanted field strength | Interfering field strength |
| ISDB-T | 90%[[17]](#footnote-17) | 10% |

#### 3.2.4.9 Protection ratios and overload threshold for interference from other services

Recommended values for protection ratios (PR) and overloading thresholdsfor ISDB-T systems to be used in sharing studies can be found in Annex 3 of Recommendation ITU-R BT.1368-13.

#### 3.2.4.10 Correction of protection ratio figures for different ACLR values

Recommendation ITU-R BT.1368-13 Attachment 3 to Annex 2 describes the calculation method to derive protection ratios for all DTTB systems for different ACLR values.

### 3.2.5 DTMB – System specific receive parameters

#### 3.2.5.1 General parameters

TABLE 28

General DTMB – VHF parameters

|  |  |
| --- | --- |
| Parameter | Fixed reception Portable reception (outdoor/Mobile or indoor) |
| Signal band width (MHz) | 7.56 |
| Thermal noise density (kT0) (dBm/Hz) | –173.98 |
| Receiver noise figure[[18]](#footnote-18) (dB) | 5 |
| Allowance for manmade noise (dB) | 1 |

#### 3.2.5.2 Carrier to noise

TABLE 29

Carrier-to-noise ratio

|  |  |
| --- | --- |
| Fixed reception | Portable reception |
| 19 dB | 14 dB |

#### 3.2.5.3 Fixed antenna system gain

For fixed reception the antenna gains used in the derivation of the minimum median field strength are given in Table 30.

Antenna gain used in the derivation of the minimum median field strength.

TABLE 30

Antenna gain used in the derivation of the minimum median field strength

|  |  |
| --- | --- |
| Band | III |
| Reference frequency (MHz) | 200 |
| Antenna gain (dBd) | 5 |
| Feeder loss (dB) | 3 |
| Antenna system gain (dBd) (1) | 2 |
| (1) Antenna system gain is equivalent to 4.15 dBi. | |

#### 3.2.5.4 Polarization discrimination fixed reception

For calculation of interference:

– For Terminal station (UE) polarization discrimination must not be applied.

– For Base Station (BS) polarization discrimination may be applied. The combined value of polarization discrimination and discrimination offered by receive aerial directivity must not be more than 12 dB[[19]](#footnote-19).

#### 3.2.5.5 Location probability – fixed reception

For fixed reception, the location probability as given in Table 31 should be used.

TABLE 31

Location Probability for fixed Reception

|  |  |
| --- | --- |
| System | DTMB |
| Location probability (%) | 95 |

#### 3.2.5.6 Portable reception definition

Portable reception is defined as:

– outdoor – which means reception by a portable receiver with an attached or built-in antenna is used outdoors at no less than 1.5 m above ground level;

– indoor – which means reception by a portable receiver with an attached or built-in antenna is used indoors at no less than 1.5 m above floor level in rooms with a window in an external wall.

In both cases, it is assumed that optimal receiving conditions will be found by moving the antenna up to 0.5 m in any direction and extreme cases, such as reception in completely shielded rooms, are disregarded.

#### 3.2.5.7 Portable receive antenna gain

Recommendation ITU-R BT.1368-13 gives in its Annex 6, § 4.1, information on antennas for portable reception. For portable reception, an omnidirectional antenna should be applied with no feeder loss. The antenna gain (relative to a half-wave dipole) is as given in Table 32.

TABLE 32

Antenna gain (dBd) for portable reception

|  |  |
| --- | --- |
| Band | Gain (dBd) |
| Band III | −2.15 |
| Note 1: Antenna gain is equivalent to 0 dBi. | |

#### 3.2.5.8 Polarization discrimination portable reception

Polarization discrimination should not be taken into account in frequency planning for fixed reception.

#### 3.2.5.9 Location probability – portable reception

For portable indoor and outdoor reception, the location probability as given in Table 33 should be used.

TABLE 33

Location probability for portable reception

|  |  |
| --- | --- |
| System | DTMB |
| Location probability (%) | 95 |

#### 3.2.5.10 Minimum field strength at 200 MHz

TABLE 34

Minimum field strength at *fr*=200 MHz

|  |  |
| --- | --- |
| Fixed reception at 10 m for  95% location probability | Portable outdoor reception at 1.5 m  for 95% location probability |
| 48.9 dBµV/m | 83.7 dBµV/m |

#### 3.2.5.11 Link budget – fixed outdoor reception

Link budgets for DTMB for fixed rooftop and portable indoor reception are provided in Annex 5.

#### 3.2.5.12 Signal time percentage

TABLE 35

Time percentages used for sharing and compatibility studies

|  |  |  |
| --- | --- | --- |
| System | Wanted field strength | Interfering field strength |
| DTMB | 50% | 1% |

# 4 Sound systems

## 4.1 Sound transmission parameters for use in sharing and compatibility studies

### 4.1.1 DAB reference broadcasting networks

Reference broadcast transmitter configurations are provided that are representative of actual deployments in the case of assignments or are the reference configurations used in the GE06 Agreement for allotment planning.

#### 4.1.1.1 DAB Single transmitter case (assignments):

– High power

• e.r.p.: 10 kW

• Effective antenna height: 300 m

• Antenna height a.g.l.: 100 m

• Antenna pattern:

○ Horizontal: Omnidirectional

○ Vertical antenna aperture: based on 12λ aperture with 2° beam tilt

– Medium power

• e.r.p.: 1 kW

• Effective antenna height: 150 m

• Antenna height a.g.l.: 50 m

• Antenna pattern:

○ Horizontal: Omnidirectional

○ Vertical: based on 6λ aperture with 3.2° beam tilt

– Low power

• e.r.p.: 50 W

• Effective antenna height: 50 m

• Antenna height a.g.l.: 20 m

• Antenna pattern:

○ Horizontal: Directional

○ Vertical: based on 2λ aperture with 6° beam tilt

The attenuation (Aϑ) of the horizontal radiation pattern with azimuth angle (ϑ) is given by:

dB

where:

where:


ϑ : azimuth angle

*k* : 0.4187 for 10 dB pattern minima.

The resulting pattern is shown in Fig. 4.

Figure 4

Low power DAB



Unlike high and medium power antennas which are usually omnidirectional, few low power DAB antenna are omnidirectional. Low power DAB antennas typically have a directional horizontal radiation pattern usually of a type cardioid (dipoles mounted on a pole) or consisting of one or more panel, Yagi or log-periodic elements. These antennas typically have minima in the HRP that are 10 dB or more below the maximum and may have lobes that occur at various azimuth angles, lobes typically being aligned with the desired service area.

As patterns of low power antenna vary considerably modelling all combinations of pattern in generic compatibility studies is usually not practical. Therefore to better represent the horizontal radiation pattern of low power DAB it is proposed to base the generic model on the pattern of a cardioid antenna with a 10 dB minimum. Depending on the compatibility study being undertaken the orientation of the pattern (angle of azimuth) can be varied as required.

#### 4.1.1.2 Vertical radiation patterns

The normalized field strength in the vicinity of the broadcast transmitting station is a function of the vertical radiation pattern of the transmitting antenna. The equation below is an approximation to be used for sharing studies.



where:



and

*A* = antenna vertical aperture in wavelengths

β = beam tilt radians below the horizontal.

Null fill is not normally applied to DAB antennas.

*E(*θ*)* given above are linear values, to convert them to reduction values in dB the following equation is used:

#### 4.1.1.3 Out of Band Mask

Information on DAB transmitter spectrum masks to be used in compatibility studies is provided in Recommendation ITU-R BS.1660.

## 4.2 Sound reception parameters for use in sharing and compatibility studies

### 4.2.1 Parameters Common to all systems

#### 4.2.1.1 Fixed antenna reference height

The reference receiving antenna height considered to be representative in calculating the field strength for fixed reception is 10 m above ground level. In order to derive the minimum median field-strength levels, the receiving antenna gain and feeder-loss values are given in Section 3.

#### 4.2.1.2 Fixed antenna radiation pattern

Standard radiation patterns for receiving antennas for Bands I, III, IV and V are as shown in Fig. 5, which are given in Recommendation [ITU-R BT.419-3](http://www.itu.int/rec/R-REC-BT.419/en).

Figure 5



#### 4.2.1.3 Portable antenna reference height

For portable (indoor and outdoor) reception, a receiving antenna height of 1.5 m above ground level is used.

#### 4.2.1.4 Polarization discrimination for portable reception

Polarization discrimination should not be taken into account in frequency planning for portable reception[[20]](#footnote-20).

#### 4.2.1.5 Height loss correction

For portable (indoor and outdoor) reception, a receiving antenna height of 1.5 m above ground level is used. The same receiving antenna height is also used for mobile reception.

However, in broadcasting, it is common practice for fixed reception to calculate the field strength at 10 m, or at the height of the surrounding clutter if it is greater than 10m, for example in an urban environment[[21]](#footnote-21). In some cases a 10m reference height is also used as the starting point in calculations for portable and mobile reception with an appropriate height loss taken into account to derive the required value at 1.5 m.

The height-loss values for portable and for mobile reception for reference frequencies are given in Table 36.

TABLE 36

Suburban and Urban height loss in Bands III[[22]](#footnote-22)

|  |  |
| --- | --- |
| Frequency (MHz) | 200 |
| Suburban height loss (dB) | 12 |
| Urban height loss (dB) | 19 |

#### 4.2.1.6 Building entry loss

The methodology described in Recommendation ITU-R P. 2109 for calculating building loss should be used in sharing and compatibility studies involving broadcast systems.

Recommendation ITU-R P.2109 covers a full range of building types of traditional and thermally efficient construction. For sharing and compatibility studies, involving broadcast systems, that use Recommendation ITU-R P.2109, whenever a single representative value is required (for example, in an MCL analysis), the parameters provided in Table 37 should be used. This is independent of coverage planning. For dynamic or statistical analysis (for example, in a Monte Carlo simulation), the full distribution function of Recommendation ITU-R P.2109 should be used.

TABLE 37

P.2109 Broadcast building entry loss parameters to use in sharing and compatibility studies

|  |  |  |
| --- | --- | --- |
| Building Type | Environment | Probability building entry loss not exceeded |
| Traditional | Suburban | 50% |
| Traditional | Urban | 70% |

NOTE – Studies of building entry loss have meant figures have changed over time with the current version of Recommendation ITU-R P.2109 representing the latest work. The parameters specified in Table 37 provide a building entry loss aligned with values derived using parameters supplied in older documents, for example Recommendation ITU-R P.1812-2.

#### 4.2.1.7 Antenna gain frequency correction

Within any frequency band, the variation of antenna gain with other frequency may be taken into account by the addition of a correction term:

where:

*Corr* : correction term

*FA* : actual working frequency being considered

*FR* : reference frequency.

Minimum median field strength levels for other frequencies are derived by interpolation as described in § 4.2.1.8.

#### 4.2.1.8 Interpolation of reference field strength values(GE06)

For frequencies other than those quoted in tables, as described in Appendix 3.5 of Chapter 3 of the Final Acts of RRC06, the reference field-strength values should be adjusted by adding the correction factor defined according to the following rule:

– (*Emed*)*ref*(*f*) = (*Emed*)*ref*(*fr*) + Corr;

– for fixed reception, Corr = 20 log10 (*f/fr*), where *f* is the actual frequency and *fr* the reference frequency in the Table;

– for portable reception and mobile reception, Corr = 30 log10 (f/fr) where f is the actual frequency and *fr* the reference frequency in the Table.

### 4.2.2 DAB – System specific receive parameters

#### 4.2.2.1 General parameters

TABLE 38

General DAB parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Outdoor | Indoor | Mobile |
| Signal band width (MHz) | 1.54 | | |
| Thermal noise density (kT0) (dBm/Hz) | –173.98 | | |
| Receiver noise figure (1) (dB) | 6 | | |
| Allowance for manmade noise (2) (dB) | 1.5 | 5.3 | 0.9 |
| (1) Report ITU-R BS.2214-3, § 7.2.1.  (2) Report ITU-R BS.2214-3, § 3.5 and Table 115. | | | |

The studies should consider three reception modes, mobile, portable outdoor and portable indoor reception.

#### 4.2.2.2 Carrier to noise

DAB system *C*/*N* values to use in sharing studies are given in Table 39.

TABLE 39

Carrier-to-noise ratio(1)

|  |  |
| --- | --- |
| Portable reception | Mobile reception |
| 11.9 dB | 12.6 |
| (1) Report ITU-R BS.2214-3, Table 115. | |

#### 4.2.2.3 Portable reception definition

Portable reception is defined as:

– outdoor – which means reception by a portable receiver with an attached or built-in antenna is used outdoors at no less than 1.5 m above ground level;

– indoor – which means reception by a portable receiver with an attached or built-in antenna is used indoors at no less than 1.5 m above floor level in rooms with a window in an external wall.

In both cases, it is assumed that optimal receiving conditions will be found by moving the antenna up to 0.5 m in any direction and extreme cases, such as reception in completely shielded rooms, are disregarded.

#### 4.2.2.4 Receive antenna gain

For portable and mobile reception, an omnidirectional antenna should be applied. The antenna gain (relative to a half-wave dipole) to use is as given in Table 40.

TABLE 40

DAB Band III Antenna gain (dBd) for portable and mobile reception(1)

|  |  |
| --- | --- |
| **Portable (dBd)** | **Mobile (dBd)** |
| –8 | –5 |
| (1) Report ITU-R BS.2214-3, Table 115.  Note: The anntena gains are equivalent to −5.85 dBi and −2.85 dBi, respectively. | |

#### 4.2.2.5 Polarization discrimination portable reception

Polarization discrimination should not be taken into account in frequency planning for portable reception.

#### 4.2.2.6 Location probability – portable reception

TABLE 41

Location probability for portable reception

|  |  |
| --- | --- |
| System | DAB (GE06) |
| Portable location probability (%) | 95 |
| Mobile location probability (%) | 99 |

#### 4.2.2.7 Minimum field strength at 200 MHz

TABLE 42

DAB Minimum field strength at fr=200 MHz

|  |  |  |
| --- | --- | --- |
| Mobile reception for 99% location probability  at 10 m a.g.l. | Portable outdoor reception for 95% location probability  at 10 m a.g.l. | Portable indoor reception for 95% location probability  at 10 m a.g.l. |
| 56.8 dBµV/m | 57 dBµV/m | 79.7 dBµV/m |

Minimum median field-strength levels for other frequencies than 200 MHz are derived by the correction described in § 4.2.1.8.

#### 4.2.2.8 Link budget – portable outdoor/indoor reception

Link budgets for DAB for mobile, portable outdoor and portable indoor reception are provided in Annex 6.

#### 4.2.2.9 Protection ratios and overload threshold for interference from other services

Recommended values for protection ratios (PR) and overloading thresholdsfor DTMB systems to be used in sharing studies can be found in Annex 4 to Recommendation ITU-R BS.1660-8.

#### 4.2.2.10 Correction of protection ratio figures for different ACLR values

Recommendation ITU-R BT.1368-13 Attachment 3 to Annex 2 describes the calculation method to derive protection ratios for all DTB systems for different ACLR values.

Annex 1  
  
List of relevant ITU-R Reports and Recommendations

Additional information on the characteristics which are referred to in this Report can be found in ITU documents:

– Recommendation [ITU-R BT.419](http://www.itu.int/rec/R-REC-BT.419/en) – Directivity and polarization discrimination of antennas in the reception of television broadcasting.

– Recommendation [ITU-R BT.500](http://www.itu.int/rec/R-REC-BT.500/en) – Methodology for the subjective assessment of the quality of television pictures.

– Recommendation [ITU-R BT.1206](http://www.itu.int/rec/R-REC-BT.1206/en) – Spectrum limit masks for digital terrestrial television broadcasting.

– Recommendation [ITU-R BT.1368](http://www.itu.int/rec/R-REC-BT.1368/en) – Planning criteria, including protection ratios, for digital terrestrial television services in the VHF/UHF bands.

– Recommendation [ITU-R BS.1660](http://www.itu.int/rec/R-REC-BS.1660/en) – Technical basis for planning of terrestrial digital sound broadcasting in the VHF band.

– Recommendation [ITU-R BT.2033](http://www.itu.int/rec/R-REC-BT.2033/en) – Planning criteria, including protection ratios, for second generation of digital terrestrial television broadcasting systems in the VHF/UHF bands.

– Report [ITU-R BT.2036](https://www.itu.int/rec/R-REC-BT.2036/en) – Characteristics of a reference receiving system for frequency planning of digital terrestrial television systems.

– Report [ITU-R BS.2214](https://www.itu.int/dms_pub/itu-r/opb/rep/R-REP-BS.2214-2-2016-MSW-E.docx) – Planning parameters for terrestrial digital sound broadcasting systems in VHF bands.

– Final Acts of RRC06 – [The GE06 Agreement](http://www.itu.int/ITU-R/index.asp?category=conferences&rlink=rrc&lang=en)[[23]](#footnote-23).

– ITU-R [DTTB Handbook](http://www.itu.int/pub/R-HDB-39).

– ITU-R [DSB Handbook.](https://www.itu.int/pub/R-HDB-20-2002)

Additional information on the characteristics which are not referred to in this Report can be found in ITU documents:

– Recommendation [ITU-R BS.774](http://www.itu.int/rec/R-REC-BS.774/en) – Service requirements for digital sound broadcasting to vehicular, portable and fixed receivers using terrestrial transmitters in the VHF/UHF bands.

– Recommendation [ITU-R BS.1114](http://www.itu.int/rec/R-REC-BS.1114/en) – Systems for terrestrial digital sound broadcasting to vehicular, portable and fixed receivers in the frequency range 30-3 000 MHz.

– Recommendation [ITU-R BS.1195](http://www.itu.int/rec/R-REC-BS.1195/en) – Transmitting antenna characteristics at VHF and UHF.

– Recommendation [ITU-R BT.1877](http://www.itu.int/rec/R-REC-BT.1877/en) – Error-correction, data framing, modulation and emission methods for second generation of digital terrestrial television broadcasting systems.

– Recommendation [ITU-R BT.1306](http://www.itu.int/rec/R-REC-BT.1306/en) – Error correction, data framing, modulation and emission methods for digital terrestrial television broadcasting.

Additional information on the protection requirements which are referred to in this Report can be found in ITU documents:

– Recommendation [ITU-R BT.1368](http://www.itu.int/rec/R-REC-BT.1368/en) – Planning criteria, including protection ratios, for digital terrestrial television services in the VHF/UHF bands.

– Recommendation [ITU-R BS.1660](http://www.itu.int/rec/R-REC-BS.1660/en) – Technical basis for planning of terrestrial digital sound broadcasting in the VHF band.

– Recommendation [ITU-R BT.1735](http://www.itu.int/rec/R-REC-BT.1735/en) – Methods for objective reception quality assessment of digital terrestrial television broadcasting signals of System B specified in Recommendation ITU-R BT.1306.

– Recommendation [ITU-R BT/BS.1895](http://www.itu.int/rec/R-REC-BT.1895/en) – Protection criteria for terrestrial broadcasting systems.

– Final Acts of RRC06 – The GE06 Agreement.

– Recommendation [ITU-R BT.2033](http://www.itu.int/rec/R-REC-BT.2033/en) – Planning criteria, including protection ratios, for second generation of digital terrestrial television broadcasting systems in the VHF/UHF bands.

– Report [ITU-R BT.2215](http://www.itu.int/pub/R-REP-BT.2215) – Measurements of Protection Ratios and Overload Thresholds for Broadcast TV Receivers.

– Report [ITU-R BT.2265](http://www.itu.int/pub/R-REP-BT.2265) – Guidelines for the assessment of interference into the broadcasting service.

– Recommendation [ITU-R BT.2036](http://www.itu.int/rec/R-REC-BT.2036/en) – Characteristics of a reference receiving system for frequency planning of digital terrestrial television systems.

Additional information on the protection requirements which are not referred to in this Report can be found in ITU documents:

– Report [ITU-R BT.2254](http://www.itu.int/pub/R-REP-BT.2254) – Frequency and network planning aspects of DVB-T2.

Information on sharing and compatibility studies involving DTB can be found in ITU documents:

– Recommendation ITU-R BT. 2136 - Assessing interference into digital terrestrial television broadcasting from other services by means of Monte Carlo simulation

– Report [ITU-R BT.2247](http://www.itu.int/pub/R-REP-BT/publications.aspx?lang=en&parent=R-REP-BT.2247) – Field measurement and analysis of compatibility between DTTB and IMT.

– Report [ITU-R BT.2248](http://www.itu.int/pub/R-REP-BT.2248-2011) – A conceptual method for the representation of loss of broadcast coverage.

– Report [ITU-R BT.2337](http://www.itu.int/pub/R-REP-BT.2337) – Sharing and compatibility studies between digital terrestrial television broadcasting and terrestrial mobile broadband applications, including IMT, in the frequency band 470-694/698 MHz.

– Report [ITU-R BT.2339](http://www.itu.int/pub/R-REP-BT.2339) – Co-channel sharing and compatibility studies between digital terrestrial television broadcasting and international mobile telecommunication in the frequency band 694‑790 MHz in the GE06 planning area.

– Report [ITU-R BT.2383](http://www.itu.int/pub/R-REP-BT.2339) – Characteristics of digital terrestrial television broadcasting systems in the frequency band 470-862 MHz for frequency sharing/interference analyses

– Report ITU-R BT.2470 – Use of Monte Carlo simulation to model interference to DTTB.

Information on propagation matters referred to in this Report can be found in ITU documents:

– Recommendation [ITU-R P.1546](http://www.itu.int/rec/R-REC-P.1546/en) – Method for point-to-area predictions for terrestrial services in the frequency range 30 MHz to 3 000 MHz.

Annex 2  
  
General definitions

## A2.1 Broadcasting coverage area and service area planning

Recommendation [ITU-R V.573-5](https://www.itu.int/rec/R-REC-V.573-5-200709-S/en) No. A51b defines “*coverage area*” as the “*area associated with a transmitting station for a given service and a specified frequency within which, under specified technical conditions, radiocommunications may be established with one or several receiving stations*”.

Note 4 of No. A51b explains that “*the term ’service area ‘should have the same technical basis as for ’coverage area‘, but also include administrative aspects*”.

Reference to the administrative aspects in the definition of service area is understood to mean that in that service area protection is required.

For the case of broadcast services which are usually planned with multiple overlapping transmissions from different transmitter sites, it is usual to protect only the best coverage. Furthermore, spill-over coverage into international neighbors or adjacent regions of a country do not usually form part of the intended service area and may not require protection.

## A2.2 Definition of reception location probability

Reception location probability is defined in Report [ITU-R BT.2265-2](http://www.itu.int/pub/R-REP-BT.2265) Section 2 as “*the percentage of locations within a small area, referred in this document as ’pixel’[[24]](#footnote-24), where the wanted signal is high enough to overcome noise and interference for a given percentage of time taking into account the temporal and spatial statistical variations of the relevant fields*”*.*

In digital terrestrial broadcasting the coverage area is defined in Report ITU-R BT.2265-2.  
Annex 2 as “*the area that comprises all pixels, where a given reference reception location probability (e.g. 95%) is reached or exceeded for a predetermined percentage of the time*”*.*

Annex 3  
  
Allotment reference networks

## A3.1 DTT Single frequency networks (Allotments)(GE06)


Three reference networks (RN) for DTT services in Region 1 will be used as described in Appendix 3.6 of Chapter 3 of the GE06 Agreement. This information is reproduced in part below.

For sharing studies within the service area of an SFN the same vertical diagrams as provided in § 7.1 above should be applied for each transmitter.

### A3.1.1 Reference network 1 (large service-area SFN)

The network consists of seven transmitters situated at the centre and at the vertices of a hexagonal lattice. An open network type has been chosen, i.e. the transmitters have non-directional antenna patterns and the service area is assumed to exceed the transmitter hexagon by about 15%. The geometry of the network is given in Fig. A3-1. This reference network (RN 1) is applied to different cases: fixed (RPC 1), outdoor/mobile (RPC 2) and indoor (RPC 3) reception, for Band III. RN 1 is intended for large service area SFN coverage. It is assumed that main transmitter sites with an appropriate effective antenna height are used as a backbone for this type of network. For portable and mobile reception, the size of the real service areas for this type of SFN coverage is restricted to 150 to 200 km in diameter because of self-interference degradation, unless very rugged DVB-T system variants are used or the concept of dense networks is employed.

FIGURE A3-1



For the guard interval length, the maximum value 1/4 *Tu* of the 8k FFT mode is assumed. The distance between transmitters in an SFN should not significantly exceed the distance equivalent to the guard interval duration. In this case, the guard interval duration is 265 μs, which corresponds to a distance of 85 km. The distance between transmitters for RPC 1 is taken as 70 km. For RPC 2 and RPC 3, 70 km is too large a distance from a power budget point of view.

Therefore, smaller values for the distance between transmitters have been selected, 50 km for RPC 2 and 40 km for RPC 3.

The parameters and the power budgets of RN 1 given in Table A3-1 should be used.

TABLE A3-1

Parameters of RN 1 (large service area SFN)

| RPC and reception type | | RPC 1 fixed antenna | RPC 2 portable outdoor and mobile | RPC 3 portable indoor |
| --- | --- | --- | --- | --- |
| Type of network | | Open | Open | Open |
| Geometry of service area | | Hexagon | Hexagon | Hexagon |
| Number of transmitters | | 7 | 7 | 7 |
| Geometry of transmitter lattice | | Hexagon | Hexagon | Hexagon |
| Distance between transmitters d (km) | | 70 | 50 | 40 |
| Service area diameter D (km) | | 161 | 115 | 92 |
| Tx effective antenna height (m) | | 150 | 150 | 150 |
| Tx antenna pattern | | Non-directional | Non-directional | Non-directional |
| e.r.p.(1) dB(W) | Band III | 34.1 | 36.2 | 40.0 |
| (1) The e.r.p. values indicated in this table incorporate an additional power margin of 3 dB. | | | | |

The e.r.p. is given for 200 MHz in Band III; for other frequencies (*f* in MHz) the frequency correction factor added is: 20 log10(*f/*200) for RPC 1 and 30 log10(*f/*200) for RPC 2 and RPC 3.

### A3.1.2 Reference network 2 (small service area SFN, dense SFN)

The network consists of three transmitters situated at the vertices of an equilateral triangle. An open network type has been chosen, i.e. the transmitters have non-directional antenna patterns. The service area is assumed to be hexagonal, as indicated in Fig. A3-2.


This reference network (RN 2) is applied to different cases: fixed (RPC 1), outdoor/mobile (RPC 2) and indoor (RPC 3) reception, for Band III.

RN 2 is intended for small service area SFN coverage. Transmitter sites with appropriate effective antenna heights are assumed to be available for this type of network and self-interference restrictions are expected to be small. Typical service area diameters may be from 30 to 50 km.

It is also possible to cover large service areas with this kind of dense SFN. However, a very large number of transmitters is then necessary. It therefore seems reasonable to have large service areas being represented by RN 1, even if a dense network structure is envisaged.

Figure A3-2

RN 2 (small service area SFN)



In RN 2 the inter-transmitter distance is 40 km for RPC 1 and 25 km in the case of RPCs 2 and 3.

The parameters and the power budgets of the RN 2 given in Table A3-2 should be used.

TABLE A3-2

Parameters of RN 2 (small service area SFN)

| RPC and reception type | | RPC 1 Fixed antenna | RPC 2 Portable outdoor and mobile | RPC 3 Portable indoor |
| --- | --- | --- | --- | --- |
| Type of network | | Open | Open | Open |
| Geometry of service area | | Hexagon | Hexagon | Hexagon |
| Number of transmitters | | 3 | 3 | 3 |
| Geometry of transmitter lattice | | Triangle | Triangle | Triangle |
| Distance between transmitters d (km) | | 40 | 25 | 25 |
| Service area diameter D (km) | | 53 | 33 | 33 |
| Tx effective antenna  height (m) | | 150 | 150 | 150 |
| Tx antenna pattern | | Non-directional | Non-directional | Non-directional |
| e.r.p.(1) (dBW) | Band III | 24.1 | 26.6 | 34.1 |
| (1) The e.r.p. values indicated in this Table incorporate an additional power margin of 3 dB. | | | | |

The e.r.p. is given for 200 MHz in Band III; for other frequencies (*f* in MHz) the frequency correction factor added is: 20 log10(*f/*200) for RPC 1 and 30 log10(*f/*200) for RPC 2 and RPC 3.

### A3.1.3 Reference network 3 (small service area SFN for urban environment)

The geometry of the transmitter lattice of reference network 3 (RN 3) and the service area are identical to those of RN 2 (see Fig. A3-2 above).

RN 3 is applied to different cases: fixed (RPC 1), outdoor/mobile (RPC 2) and indoor (RPC 3) reception, for Band III.

RN 3 is intended for small service area SFN coverage in an urban environment. It is identical to RN 2, apart from the fact that urban-type height loss figures are used. This increases the required power of the SFN transmitters by about 5 dB for RPC 2 and RPC 3.

The parameters and the power budgets of the RN 3 given in Table A3-3 should be used.

TABLE A3-3

Parameters of RN 3 (small service area SFN for urban environment)

| RPC and reception type | | RPC 1 fixed antenna | RPC 2 portable outdoor and mobile | RPC 3 portable indoor |
| --- | --- | --- | --- | --- |
| Type of network | | Open | Open | Open |
| Geometry of service area | | Hexagon | Hexagon | Hexagon |
| Number of transmitters | | 3 | 3 | 3 |
| Geometry of transmitter lattice | | Triangle | Triangle | Triangle |
| Distance between transmitters d (km) | | 40 | 25 | 25 |
| Service area diameter D (km) | | 53 | 33 | 33 |
| Tx effective antenna height (m) | | 150 | 150 | 150 |
| Tx antenna pattern | | Non-directional | Non-directional | Non-directional |
| e.r.p.(1) (dBW) | Band III | 24.1 | 32.5 | 40.1 |
| (1) The e.r.p. values indicated in this Table incorporate an additional power margin of 3 dB. | | | | |

The e.r.p. is given for 200 MHz in Band III; for other frequencies (*f* in MHz) the frequency correction factor added is: 20 log10(*f*/200) for RPC 1 and 30 log10(*f*/200) for RPC 2 and RPC 3.

## A3.2 DSB Single frequency networks (Allotments)(GE06)

Two reference networks (RN) for DAB services in Region 1 will be used as described in Appendix 3.6 of Chapter 3 of the GE06 Agreement. This information is reproduced in part below.

For sharing studies within the service area of an SFN the same vertical diagrams as provided in § 7.1.1 based on the aperture and beam tilt in § 7.3 above should be applied for each transmitter.

### A3.2.1 Reference networks for DAB(GE06)

For DAB, two RPCs have been defined, RPC 4 for the mobile reception case and RPC 5 for the portable indoor reception case. Two corresponding reference networks have been designed which are identical apart from their power budget. They are directly connected to the two RPCs.

For RPC 4, the mobile reception case, the reference network consists of seven transmitters located at the centre and the vertices of a hexagon and is of the closed network type. The power of the central transmitter is reduced by 10 dB with respect to the peripheral transmitters, which have a power of 1 kW. The antenna patterns of the peripheral transmitters have a reduction of the outgoing field strength of 12 dB over 240°. A sharp transition from 0 dB to 12 dB reduction is assumed at the indicated bearings.

TABLE A3-4

Parameters of RN 5 for RPC 4 and RN 6 for RPC 5

| RPC | RPC 4 | RPC 5 |
| --- | --- | --- |
| Reception type | Mobile | Portable indoor |
| Type of network | Closed | closed |
| Geometry of service area | Hexagon | Hexagon |
| Number of transmitters | 7 | 7 |
| Geometry of transmitter lattice | Hexagon | Hexagon |
| Distance between transmitters *d* (km) | 60 | 60 |
| Service area diameter *D* (km) | 120 | 120 |
| Tx effective antenna height (m) | 150 | 150 |
| Peripheral Tx antenna pattern | Directional 12 dB reduction  over 240° | Directional 12 dB reduction  over 240° |
| Central Tx antenna pattern | Non-directional | Non-directional |
| Peripheral Tx e.r.p. (dBW) | 30.0 | 39.0 |
| Central Tx e.r.p. (dBW) | 20.0 | 29.0 |
| The e.r.p. is given for 200 MHz; for other frequencies (*f* in MHz) the frequency correction factor to be added is: 30 log10 (*f*/200) for RPC 4 and RPC 5. | | |

For RPC 5, the portable indoor reception case, the same reference network characteristics are used as for RPC 4, apart from the transmitter powers which are increased by 9 dB, corresponding to the higher minimum field strength needed for this reception mode.

The parameters and the power budgets of the RN 5 for RPC 4 and RN 6 for RPC 5 given in Table A3‑4 should be used. Figure A3-3 shows the geometry of the RNs.

Figure A3-3

Geometry of the RNs for T-DAB



Annex 4  
  
Calculation of minimum field strength and minimum   
median equivalent field strength

The minimum field strength and minimum median equivalent field strengthvalues calculated using the following equations:

*Pn* = *F* + 10 log (*k T*0 *B*)

*Ps min* = *C*/*N* + *Pn*

*Aa*= *G* + 10 log (1.64λ2/4 π)

φ*min* = *Ps min* – *Aa*+ *Lf*

*Emin* = φ*min* + 120 + 10 log (120 π)

= φ*min* + 145.8

*Emed*= *Emin* + *Pmmn* + *C*l for roof top level fixed reception

*Emed*= *Emin* + *Pmmn* + *C*l + *Lh*for portable outdoor and mobile reception

*Emed*= *Emin* + *Pmmn* + *C*l + *Lh* + *Lb*for portable indoor and mobile hand-held reception

*Cl* = µ ⋅ σ*t*

σ*t* = 

where:

*Pn* : receiver noise input power (dBW)

*F* : receiver noise figure (dB)

*k* : Boltzmann’s constant (*k* = 1.38 × 10–23 (J/K))

*T*0 : absolute temperature (*T*0 = 290 (K))

*B* : receiver noise bandwidth (*B* = 7.61 × 106 (Hz))

*Ps min* : minimum receiver input power (dBW)

*C*/*N* : RF *S*/*N* at the receiver input required by the system (dB)

*Aa* : effective antenna aperture (dBm2)

*G* : antenna gain related to half dipole (dBd)

λ : wavelength of the signal (m)

φ*min* : minimum pfd at receiving place (dB(W/m2))

*Lf* : feeder loss (dB)

*Emin* : equivalent minimum field strength at receiving place (dB(μV/m))

*Emed* : minimum median equivalent field strength, planning value (dB(μV/m))

*Pmmn* : allowance for man-made noise (dB)

*Lh* : height loss (reception point at 1.5 m above ground level) (dB)

*Lb* : building or vehicle entry loss (dB)

*Cl*: location correction factor (dB)

σ*t* :total standard deviation (dB)

σ*m* :standard deviation macro-scale (σ*m* = 5.5 (dB))

σ*b* :standard deviation building entry loss (dB)

µ :distribution factor being 0.52 for 70%, 1.28 for 90%, 1.64 for 95% and 2.33 for 99%.

Annex 5  
  
DTTB link budgets

## A5.1 DVB-T

### A5.1.1 DVB-T Fixed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DVB-T link budget for fixed roof top reception | | | | | |
| DVB-T transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and  0.25 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DVB-T receiver parameters | | | | | |
| **Rx antenna height** | m | 10.00 | 10.00 | 10.00 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 7.00 | 7.00 | 7.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 6.66 | 6.66 | 6.66 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 5 | 5 | 5 | ITU-R BT.1368-13 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 2 | 2 | 2 | Table 9 |
| **Noise power (Pn)** | dBm | –98.74 | –98.74 | –98.74 | Pn(dBm) = F+10log(k\*T\*B\*106)+30 |
| **SNR at cell edge** | dB | 20 | 20 | 20 | Table 10 |
| **Receiver sensitivity (Pmin)** | dBm | –78.74 | –78.74 | –78.74 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 8 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R 1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 95% \*  |
| **Pmean (95%)** | dBm | –69.72 | –69.72 | –69.72 | Pmean = Pmin + Lm |
| **Minimum field strength  at receive antenna** | dBµV/m | 46.39 | 46.39 | 46.39 |  |
| **Feeder loss (Lcable)** | dB | 2.00 | 2.00 | 2.00 | Table 7 |
| **Antenna gain (Giso)** | dBi | 9.15 | 9.15 | 9.15 | Table 7 |
| **Giso** – **Lcable** | dBi | 7.15 | 7.15 | 7.15 | Table 7 |
| **Max allowed path loss (Lp)** | dB | 152 | 142 | 133 | Lp = EIRP + (Giso – Lcable) – Pmean |

### A5.1.2 DVB-T portable outdoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DVB-T link budget for portable outdoor reception | | | | | |
| DVB-T transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and  0.25 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DVB-T receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 7.00 | 7.00 | 7.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 6.66 | 6.66 | 6.66 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 5 | 5 | 5 | ITU-R BT.1368-13 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 8 | 8 | 8 | Table 5 |
| **Noise power (Pn)** | dBm | –92.74 | –92.74 | –92.74 | Pn(dBm) = F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 18 | 18 | 18 | Table 10 |
| **Receiver sensitivity (Pmin)** | dBm | –74.74 | –74.74 | –74.74 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 10 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R 1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 95% \*  |
| **Pmean (95%)** | dBm | –65.72 | –65.72 | –65.72 | Pmean = Pmin + Lm |
| **Minimum field strength at 20 m** | dBµV/m | 76.5 | 76.5 | 76.5 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 69.5 | 69.5 | 69.5 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | 0.00 | 0.00 | 0.00 | Table 9 |
| **Giso** – **Lcable** | dBi | 0.00 | 0.00 | 0.00 |  |
| **Urban height loss 20 m to 1.5 m (**Lheight) | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban height loss 10 m to 1.5 m (**Lheight) | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban 20m max path loss (Lp)** | dB | 121 | 111 | 102 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |
| **Suburban 10m max path loss (Lp)** | dB | 128 | 118 | 109 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |

### A5.1.3 DVB-T portable indoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DVB-T link budget for portable indoor reception | | | | | |
| DVB-T transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and  0.25 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DVB-T receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 7.00 | 7.00 | 7.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 6.66 | 6.66 | 6.66 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 5 | 5 | 5 | ITU-R BT.1368-13 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 8 | 8 | 8 | Table 5 |
| **Noise power (Pn)** | dBm | –92.74 | –92.74 | –92.74 | Pn(dBm) = F+10log(k\*T\*B\*106)+30 |
| **SNR at cell edge** | dB | 18 | 18 | 18 | Table 10 |
| **Receiver sensitivity (Pmin)** | dBm | –74.74 | –74.74 | –74.74 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 10 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 95% \*  |
| **Pmean (95%)** | dBm | –65.72 | –65.72 | –65.72 | Pmean = Pmin + Lm |
| **Minimum field strength at 20 m** | dBµV/m | 94.10 | 94.10 | 94.10 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 83.50 | 83.50 | 83.50 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | 0.00 | 0.00 | 0.00 | Table 9 |
| **Giso** – **Lcable** | dBi | 0.00 | 0.00 | 0.00 |  |
| **Urban Height Loss 20 m to 1.5 m (**Lheight) | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban Height Loss 10 m to 1.5 m (**Lheight) | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban Building Entry Loss** (p=70%) (*Lwall*) | dB | 17.6 | 17.6 | 17.6 | Table 4 |
| Suburban Building Entry Loss (p=50%)(*Lwall*) | dB | 14 | 14 | 14 | Table 4 |
| **Urban 20m max path loss (Lp)** | dB | 104 | 94 | 85 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |
| Suburban 10m max path loss (Lp) | dB | 114 | 104 | 95 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |

## A5.2 DVB-T2

### A5.2.1 DVB-T2 Fixed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DVB-T2 link budget for fixed roof top reception | | | | | |
| DVB-T2 transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and  0.25 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DVB-T2 receiver parameters | | | | | |
| **Rx antenna height** | m | 10.00 | 10.00 | 10.00 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.2033-1 |
| **Channel BW** | MHz | 7.00 | 7.00 | 7.00 | ITU-R BT.2033-1 |
| **Effective BW** | MHz | 6.66 | 6.66 | 6.66 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 6 | 6 | 6 | ITU-R BT.2033-1 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 2 | 2 | 2 | Table 5 |
| **Noise power (Pn)** | dBm | –97.74 | –97.74 | –97.74 | Pn(dBm) = F+10log(k\*T\*B\*106)+30 |
| **SNR at cell edge** | dB | 20 | 20 | 20 | Table 6 |
| **Receiver sensitivity (Pmin)** | dBm | –77.74 | –77.74 | –77.74 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 8 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 95% \*  |
| **Pmean (95%)** | dBm | –68.72 | –68.72 | –68.72 | Pmean = Pmin + Lm |
| **Minimum field strength  at receive antenna** | dBµV/m | 47.35 | 47.35 | 47.35 |  |
| **Feeder loss (Lcable)** | dB | 2.00 | 2.00 | 2.00 | Table 7 |
| **Antenna gain (Giso)** | dBi | 9.15 | 9.15 | 9.15 | Table 7 |
| **Giso** – **Lcable** | dBi | 7.15 | 7.15 | 7.15 | Table 7 |
| **Max allowed path loss (Lp)** | dB | 151 | 141 | 132 | Lp = EIRP + (Giso – Lcable)– Pmean |

### A5.2.2 DVB-T2 outdoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DVB-T2 link budget for portable outdoor reception | | | | | |
| DVB-T2 transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and  0.25 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DVB-T2 receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.2033-1 |
| **Channel BW** | MHz | 7.00 | 7.00 | 7.00 | ITU-R BT.2033-1 |
| **Effective BW** | MHz | 6.66 | 6.66 | 6.66 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 6 | 6 | 6 | ITU-R BT.2033-1 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 8 | 8 | 8 | Table 5 |
| **Noise power (Pn)** | dBm | –91.74 | –91.74 | –91.74 | Pn(dBm) = F+10log(k\*T\*B\*106)+30 |
| **SNR at cell edge** | dB | 18 | 18 | 18 | Table 6 |
| **Receiver sensitivity (Pmin)** | dBm | –73.74 | –73.74 | –73.74 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 10 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Building entry loss standard deviation (w)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Total loss standard deviation (T)** | dB | 5.50 | 5.50 | 5.50 | sT = SQRT(2 + w2) |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 95% \*  |
| **Pmean (95%)** | dBm | –64.72 | –64.72 | –64.72 | Pmean = Pmin + Lm |
| **Minimum field strength at 10 m** | dBµV/m | 77.50 | 77.50 | 77.50 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 70.50 | 70.50 | 70.50 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | 0.00 | 0.00 | 0.00 | Table 9 |
| **Giso** – **Lcable** | dBi | 0.00 | 0.00 | 0.00 |  |
| **Urban height loss 10 m to 1.5 m (**Lheight**)** | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban height loss 10 m to 1.5 m (**Lheight**)** | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban 20 m max path loss (Lp)** | dB | 120 | 110 | 101 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |
| **Suburban 10m max path loss (Lp)** | dB | 127 | 117 | 108 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |

### A5.2.3 DVB-T2 indoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DVB-T2 link budget for portable indoor reception | | | | | |
| DVB-T2 transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and  0.25 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DVB-T2 receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.2033-1 |
| **Channel BW** | MHz | 7.00 | 7.00 | 7.00 | ITU-R BT.2033-1 |
| **Effective BW** | MHz | 6.66 | 6.66 | 6.66 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 6 | 6 | 6 | ITU-R BT.2033-1 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for man made noise** | dB | 8 | 8 | 8 | Table 5 |
| **Noise power (Pn)** | dBm | –91.74 | –91.74 | –91.74 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 18 | 18 | 18 | Table 10 |
| **Receiver sensitivity (Pmin)** | dBm | –73.74 | –73.74 | –73.74 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 10 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 95% \*  |
| **Pmean (95%)** | dBm | –64.72 | –64.72 | –64.72 | Pmean = Pmin + Lm |
| **Minimum field strength at 20 m** | dBµV/m | 95.10 | 95.10 | 95.10 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 84.50 | 84.50 | 84.50 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | 0.00 | 0.00 | 0.00 | Table 9 |
| **Giso** – **Lcable** | dBi | 0.00 | 0.00 | 0.00 |  |
| **Urban height loss 10 m to 1.5 m (**Lheight**)** | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban height loss 10 m to 1.5 m (**Lheight**)** | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban building entry loss (P=70%)(** Lwall**)** | dB | 17.6 | 17.6 | 17.6 | Table 4 |
| **Suburban building entry loss (P=50%)(** Lwall**)** | dB | 14 | 14 | 14 | Table 4 |
| **Urban 20m max path loss (Lp)** | dB | 103 | 93 | 84 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |
| **Suburban 10m max path loss (Lp)** | dB | 113 | 103 | 94 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |

## A5.3 ATSC

### A5.3.1 ATSC fixed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ATSC link budget for fixed roof top reception | | | | | |
| ATSC transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 84.19 | 76.92 | 72.15 | For 160 kW, 30 kW and 10 kW ERP transmitters respectively |
| **Antenna height above average terrain** | m | 305.00 | 610.00 | 1000.00 | § 3.1.2.1 |
| ATSC receiver parameters | | | | | |
| **Rx antenna height** | m | 10.00 | 10.00 | 10.00 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 6.00 | 6.00 | 6.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 6 | 6 | 6 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 10 | 10 | 10 | Table 14 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 0 | 0 | 0 | Table 14 |
| **Noise power (Pn)** | dBm | –96.19 | –96.19 | –96.19 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 15 | 15 | 15 | Table 15 |
| **Receiver sensitivity (Pmin)** | dBm | –81.19 | –81.19 | –81.19 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 50 | 50 | 50 | Table 17 |
| **Gaussian confidence factor for cell edge coverage probability of 50% (50%)** | % | 0.00 | 0.00 | 0.00 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Loss margin (Lm) 50%** | dB | 0.00 | 0.00 | 0.00 | Lm = 50% \*  |
| **Pmean (50%)** | dBm | –81.20 | –81.20 | –81.20 | Pmean = Pmin + Lm |
| **Minimum field strength at 10 m** | dBµV/m | 35.87 | 35.87 | 35.87 |  |
| **Feeder loss (Lcable)** | dB | 2.00 | 2.00 | 2.00 | Table 16 |
| **Antenna gain (Giso)** | dBi | 8.15 | 8.15 | 8.15 | Table 16 |
| **Giso** – **Lcable** | dBi | 6.15 | 6.15 | 6.15 | Table 16 |
| **Max allowed path loss (Lp)** | dB | 171.53 | 164.26 | 159.49 | Lp = EIRP + (Giso – Lcable) –Pmean |

### A5.3.2 ATSC outdoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ATSC link budget for portable outdoor reception | | | | | |
| ATSC transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 84.19 | 76.92 | 72.15 | For 160 kW, 30 kW and 10 kW ERP transmitters respectively |
| **Antenna height above average terrain** | m | 305.00 | 610.00 | 1000.00 | § 3.1.2.1 |
| ATSC receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BT.2036-2 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 6.00 | 6.00 | 6.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 6 | 6 | 6 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 10 | 10 | 10 | Table 14 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 0 | 0 | 0 | Table 18 |
| **Noise power (Pn)** | dBm | –96.19 | –96.19 | –96.19 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 15 | 15 | 15 |  |
| **Receiver sensitivity (Pmin)** | dBm | –81.20 | –81.20 | –81.20 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 50 | 50 | 50 | Table 19 |
| **Gaussian confidence factor for cell edge coverage probability of 50% (50%)** | % | 0.00 | 0.00 | 0.00 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Loss margin (Lm) 50%** | dB | 0.00 | 0.00 | 0.00 | Lm = 50% \*  |
| **Pmean (50%)** | dBm | –81.20 | –81.20 | –81.20 | Pmean = Pmin + Lm |
| **Minimum field strength at 20 m** | dBµV/m | 61.02 | 61.02 | 61.02 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 54.02 | 54.02 | 54.02 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | 0.00 | 0.00 | 0.00 | Tabe 18 |
| **Giso** – **Lcable** | dBi | 0.00 | 0.00 | 0.00 |  |
| **Urban height loss 10 m to 1.5m (**Lheight**)** | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban height loss 10 m to 1.5 m (**Lheight**)** | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban 20m max path loss (Lp)** | dB | 146 | 139 | 134 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |
| **Suburban 10m max path loss (Lp)** | dB | 153 | 146 | 141 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |

## A5.4 ISDB-T

### A5.4.1 ISDB-T fixed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ISDB-T link budget for fixed roof top reception | | | | | |
| ISDB-T transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 74.19 | 64.19 | 54.19 | For 16 kW, 1.6 kW and 0.16 kW ERP transmitters respectively |
| **Antenna height above average terrain** | m | 150.00 | 150.00 | 150.00 | § 3.1.3.1 |
| ISDB-T receiver parameters | | | | | |
| **Rx Antenna height** | m | 10.00 | 10.00 | 10.00 | ITU-R BT.2036-2 |
| **Center frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 6.00 | 6.00 | 6.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 5.6 | 5.6 | 5.6 | ITU-R BT.1368-13 |
| **Noise figure (F)** | dB | 5 | 5 | 5 | ITU-R BT.1368-13 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 1 | 1 | 1 | ITU-R BT.1368-13 |
| **Noise power (Pn)** | dBm | –100.49 | –100.49 | –100.49 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 20.1 | 20.1 | 20.1 | ITU-R BT.2036-2 |
| **Receiver sensitivity (Pmin)** | dBm | –80.39 | –80.39 | –80.39 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 |  |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = % \*  |
| **Pmean (95%)** | dBm | –71.37 | –71.37 | –71.37 | Pmean = Pmin + Lm |
| **Minimum field strength at 10 m** | dBµV/m | 47.71 | 47.71 | 47.71 |  |
| **Feeder loss (Lcable)** | dB | 3.00 | 3.00 | 3.00 | Table 24 |
| **Antenna gain (Giso)** | dBi | 7.15 | 7.15 | 7.15 | Table 24 |
| **Giso** – **Lcable** | dBi | 4.15 | 4.15 | 4.15 | Table 24 |
| **Max allowed path loss (Lp)** | dB | 149.71 | 139.71 | 129.71 | Lp = EIRP + (Giso – Lcable) – Pmean |

## A5.5 DTMB

### A5.5.1 DTMB fixed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DTMB link budget for fixed roof top reception | | | | | |
| DTMB transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and 0.25 kW ERP transmitters respectively |
| **Tx Antenna Effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DTMB receiver parameters | | | | | |
| **Rx Antenna height** | m | 10.00 | 10.00 | 10.00 | ITU-R BT.2036-2 |
| **Center frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 8.00 | 8.00 | 8.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 7.56 | 7.56 | 7.56 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 5 | 5 | 5 | ITU-R BT.1368-13 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 1 | 1 | 1 | Table 28 |
| **Noise power (Pn)** | dBm | –99.19 | –99.19 | –99.19 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 19 | 19 | 19 | Table 33 |
| **Receiver sensitivity (Pmin)** | dBm | –80.19 | –80.19 | –80.19 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 31 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (5%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Building entry loss standard deviation (w)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Total loss standard deviation (T)** | dB | 5.50 | 5.50 | 5.50 | sT = SQRT(2 + w2) |
| **Loss margin (Lm)** | 50% | 9.02 | 9.02 | 9.02 | Lm = 5% \*  |
| **Pmean (95%)** | dBm | –71.17 | –71.17 | –71.17 | Pmean = Pmin + Lm |
| **Minimum field strength at 10 m** | dBµV/m | 47.91 | 47.91 | 47.91 |  |
| **Feeder loss (Lcable)** | dB | 3.00 | 3.00 | 3.00 | Table 30 |
| **Antenna gain (Giso)** | dBi | 7.15 | 7.15 | 7.15 | Table 30 |
| **Giso** – **Lcable** | dBi | 4.15 | 4.15 | 4.15 | Table 30 |
| **Max allowed path loss (Lp)** | dB | 150 | 140 | 131 | Lp = EIRP + (Giso – Lcable) – Pmean |

### A5.5.2 DTMB indoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DTMB link budget for portable indoor reception | | | | | |
| DTMB transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 75.16 | 65.16 | 56.13 | For 20 kW, 2 kW and 0.25 kW ERP transmitters respectively |
| **Tx Antenna Effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DTMB receiver parameters | | | | | |
| **Rx Antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BT.2036-2 |
| **Center frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BT.1368-13 |
| **Channel BW** | MHz | 8.00 | 8.00 | 8.00 | ITU-R BT.1368-13 |
| **Effective BW** | MHz | 7.56 | 7.56 | 7.56 | ITU-R BT.2036-2 |
| **Noise figure (F)** | dB | 5 | 5 | 5 | ITU-R BT.1368-13 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 1 | 1 | 1 | Table 28 |
| **Noise power (Pn)** | dBm | –99.19 | –99.19 | –99.19 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 14 | 14 | 14 | Table 29 |
| **Receiver sensitivity (Pmin)** | dBm | –85.19 | –85.19 | –85.19 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 |  |
| **Gaussian confidence factor for cell edge coverage probability of 95% (5%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R P.1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 95% \*  |
| **Pmean (95%)** | dBm | –76.17 | –76.17 | –76.17 | Pmean = Pmin + Lm |
| **Minimum field strength at 20 m** | dBµV/m | 83.65 | 83.65 | 83.65 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 73.05 | 73.05 | 73.05 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | 0.00 | 0.00 | 0.00 |  |
| **Giso** – **Lcable** | dBi | 0.00 | 0.00 | 0.00 |  |
| **Urban Height Loss 20 m to 1.5 m (**Lheight**)** | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban Height Loss 10 m to 1.5 m (**Lheight**)** | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban Building Entry Loss (P=70%)(** Lwall**)** | dB | 17.6 | 17.6 | 17.6 | Table 4 |
| **Suburban Building Entry Loss (P=50%)(** Lwall**)** | dB | 14 | 14 | 14 | Table 4 |
| **Urban 20m max path loss (Lp)** | dB | 114 | 104 | 95 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |
| **Suburban 10m max path loss (Lp)** | dB | 125 | 115 | 106 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |

Annex 6  
  
DSB link budgets

## A6.1 DAB

### A6.1.1 DAB mobile

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DAB link budget for mobile reception | | | | | |
| DAB transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 72.15 | 62.15 | 49.14 | For 10 kW, 1 kW and 0.05 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DAB receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BS.2214-3 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BS.2214-3 |
| **Channel BW** | MHz | 1.75 | 1.75 | 1.75 | ITU-R BS.1660-8 |
| **Effective BW** | MHz | 1.54 | 1.54 | 1.54 | ITU-R BS.1660-8 |
| **Noise figure (F)** | dB | 6 | 6 | 6 | ITU-R BS.2214-3 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for man-made noise** | dB | 0.9 | 0.9 | 0.9 | ITU-R BS.2214-3 |
| **Noise power (Pn)** | dBm | -105.20 | -105.20 | -105.20 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 12.6 | 12.6 | 12.6 | ITU-R BS.2214-3 |
| **Receiver sensitivity (Pmin)** | dBm | –92.60 | –92.60 | –92.60 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 99 | 99 | 99 | Table 41 |
| **Gaussian confidence factor for cell edge coverage probability of 99% (99%)** | % | 2.33 | 2.33 | 2.33 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R 1546-6 |
| **Loss margin (Lm) 99%** | dB | 12.82 | 12.82 | 12.82 | Lm = 99% \*  |
| **Pmean (99%)** | dBm | –79.78 | –79.78 | –79.78 | Pmean = Pmin + Lm |
| **Minimum field strength at 10 m** | dBµV/m | 65.30 | 65.30 | 65.30 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 58.30 | 58.30 | 58.30 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | –2.85 | –2.85 | –2.85 | ITU-R BS.2214-3 |
| **Giso** – **Lcable** | dBi | –2.85 | –2.85 | –2.85 |  |
| **Urban height loss 20 m to 1.5 m (**Lheight**)** | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban height loss 10 m to 1.5 m (**Lheight**)** | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban 20m max path loss (Lp)** | dB | 130 | 120 | 107 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |
| **Suburban 10m max path loss (Lp)** | dB | 137 | 127 | 114 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |

### A6.1.2 DAB portable indoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DAB link budget for portable indoor reception | | | | | |
| DAB transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 72.15 | 62.15 | 49.14 | For 10 kW, 1 kW and 0.05 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DAB receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BS.2214-3 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BS.2214-3 |
| **Channel BW** | MHz | 1.75 | 1.75 | 1.75 | ITU-R BS.1660-8 |
| **Effective BW** | MHz | 1.54 | 1.54 | 1.54 | ITU-R BS.1660-8 |
| **Noise figure (F)** | dB | 6 | 6 | 6 | ITU-R BS.2214-3 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 5.3 | 5.3 | 5.3 | ITU-R BS.2214-3 |
| **Noise power (Pn)** | dBm | –100.80 | –100.80 | –100.80 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 11.9 | 11.9 | 11.9 | ITU-R BS.2214-3 |
| **Receiver sensitivity (Pmin)** | dBm | –88.90 | –88.90 | –88.90 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 41 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R 1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 99% \*  |
| **Pmean (95%)** | dBm | –79.88 | –79.88 | –79.88 | Pmean = Pmin + Lm |
| **Minimum field strength at 20 m** | dBµV/m | 85.79 | 85.79 | 85.79 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 75.19 | 75.19 | 75.19 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | –5.85 | –5.85 | –5.85 | ITU-R BS.2214-3 |
| **Giso** – **Lcable** | dBi | –5.85 | –5.85 | –5.85 |  |
| **Urban height loss 20 m to 1.5 m (**Lheight**)** | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban height loss 10 m to 1.5 m (**Lheight**)** | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban Building entry loss (P=70%)(** Lwall**)** | dB | 17.6 | 17.6 | 17.6 | Table 37 |
| **Suburban Building entry loss (P=50%)(** Lwall**)** | dB | 14 | 14 | 14 | Table 37 |
| **Urban 20m max path loss (Lp)** | dB | 109 | 99 | 86 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |
| **Suburban 10m max path loss (Lp)** | dB | 120 | 109 | 97 | Lp = EIRP + (Giso – Lcable) – Lwall – Lheight – Pmean |

### A6.1.3 DAB portable outdoor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DAB link budget for portable outdoor reception | | | | | |
| DAB transmitter parameters | | | | | |
|  | Unit | High power transmitter | Medium power transmitter | Low power transmitter | Notes |
| **EIRP** | dBm | 72.15 | 62.15 | 49.14 | For 10 kW, 1 kW and 0.05 kW ERP transmitters respectively |
| **Tx antenna effective height** | m | 300.00 | 150.00 | 70.00 |  |
| DAB receiver parameters | | | | | |
| **Rx antenna height** | m | 1.50 | 1.50 | 1.50 | ITU-R BS.2214-3 |
| **Centre frequency** | MHz | 200.00 | 200.00 | 200.00 | ITU-R BS.2214-3 |
| **Channel BW** | MHz | 1.75 | 1.75 | 1.75 | ITU-R BS.1660-8 |
| **Effective BW** | MHz | 1.54 | 1.54 | 1.54 | ITU-R BS.1660-8 |
| **Noise figure (F)** | dB | 6 | 6 | 6 | ITU-R BS.2214-3 |
| **Boltzmann's constant (k)** | J/K | 1.38E-23 | 1.38E-23 | 1.38E-23 |  |
| **Absolute temperature (T)** | K | 290 | 290 | 290 |  |
| **Allowance for manmade noise** | dB | 1.5 | 1.5 | 1.5 | ITU-R BS.2214-3 |
| **Noise power (Pn)** | dBm | –104.60 | –104.60 | –104.60 | Pn(dBm) =  F + 10log(k\*T\*B\*106) + 30 |
| **SNR at cell edge** | dB | 11.9 | 11.9 | 11.9 | ITU-R BS.2214-3 |
| **Receiver sensitivity (Pmin)** | dBm | –92.70 | –92.70 | –92.70 | Pmin = Pn(dBm) + SNR(dB) |
| **Cell edge coverage probability** | % | 95 | 95 | 95 | Table 41 |
| **Gaussian confidence factor for cell edge coverage probability of 95% (95%)** | % | 1.64 | 1.64 | 1.64 |  |
| **Shadowing loss standard deviation ()** | dB | 5.50 | 5.50 | 5.50 | ITU-R 1546-6 |
| **Loss margin (Lm) 95%** | dB | 9.02 | 9.02 | 9.02 | Lm = 99% \*  |
| **Pmean (95%)** | dBm | –83.68 | –83.68 | –83.68 | Pmean = Pmin + Lm |
| **Minimum field strength at 10 m** | dBµV/m | 64.40 | 64.40 | 64.40 | Urban |
| **Minimum field strength at 10 m** | dBµV/m | 57.40 | 57.40 | 57.40 | Suburban |
| **Feeder loss (Lcable)** | dB | 0.00 | 0.00 | 0.00 |  |
| **Antenna gain (Giso)** | dBi | –5.85 | –5.85 | –5.85 | ITU-R BS.2214-3 |
| **Giso** – **Lcable** | dBi | –5.85 | –5.85 | –5.85 |  |
| **Urban height loss 20 m to 1.5 m (L**height**)** | dB | 19 | 19 | 19 | ITU-R P.1546-6 |
| **Suburban height loss 10 m to 1.5 m (L**height**)** | dB | 12 | 12 | 12 | ITU-R P.1546-6 |
| **Urban 20 m max path loss (Lp)** | dB | 131 | 121 | 109 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |
| **Urban 20 m max path loss (Lp)** | dB | 138 | 128 | 115 | Lp = EIRP + (Giso – Lcable) – Lheight – Pmean |

1. Characteristics of Band IV/V broadcast systems can be found in Report ITU-R BT.2383 – Typical frequency sharing characteristics of digital terrestrial television systems in the frequency band 470‑862 MHz. [↑](#footnote-ref-1)
2. Time availability in this case refers to the time that a service is not subject to interference due to enhanced propagation conditions. [↑](#footnote-ref-2)
3. Refer to Recommendations [ITU-R BT.500](http://www.itu.int/rec/R-REC-BT.500/en), [ITU-R BT.1735](http://www.itu.int/rec/R-REC-BT.1735/en) and [ITU-R BS.1284](https://www.itu.int/rec/R-REC-BS.1284/en). [↑](#footnote-ref-3)
4. Report ITU-R BT.2470 ‒ Use of Monte Carlo simulation to model interference to DTTB. [↑](#footnote-ref-4)
5. Recommendation ITU-R BT.2136 ‒ Assessing interference into digital terrestrial television broadcasting from other services by means of Monte Carlo simulation. [↑](#footnote-ref-5)
6. Refer to Report [ITU-R BT.2248](http://www.itu.int/pub/R-REP-BT.2248). [↑](#footnote-ref-6)
7. Values are derived from the Consolidated Data Base System (CDBS) found at:  
   <http://transition.fcc.gov/ftp/Bureaus/MB/Databases/cdbs/index.html>. [↑](#footnote-ref-7)
8. See: <http://transition.fcc.gov/Bureaus/Engineering_Technology/Documents/bulletins/oet69/oet69.pdf>. [↑](#footnote-ref-8)
9. Recommendations [ITU-R BT.1368-13](https://www.itu.int/rec/R-REC-BT.1368-13-201706-I/en) and [ITU-R BT.2033-1](https://www.itu.int/rec/R-REC-BT.2033/en). [↑](#footnote-ref-9)
10. See Recommendation ITU-R P.1546-6, Annex 5 § 9. [↑](#footnote-ref-10)
11. Refer to Recommendation [ITU-R P.1546](http://www.itu.int/rec/R-REC-P.1546/en)-5. They are equivalent to the values provided in GE06. [↑](#footnote-ref-11)
12. Also referred to as variability due to shadowing – shadow loss fading. [↑](#footnote-ref-12)
13. Refer to Recommendation [ITU-R BT 419-3](http://www.itu.int/rec/R-REC-BT.419/en). [↑](#footnote-ref-13)
14. Recommendation [ITU-R BT.1368-13](https://www.itu.int/rec/R-REC-BT.1368/en). [↑](#footnote-ref-14)
15. Recommendation [ITU-R BT.1368-13](http://www.itu.int/pub/R-REP-BT.1368). [↑](#footnote-ref-15)
16. . [↑](#footnote-ref-16)
17. . [↑](#footnote-ref-17)
18. Refer to Recommendation [ITU-R BT.1368-13](https://www.itu.int/rec/R-REC-BT.1368/en), Annex 2. [↑](#footnote-ref-18)
19. Refer to Recommendation [ITU-R BT.419-3](http://www.itu.int/rec/R-REC-BT.419/en). [↑](#footnote-ref-19)
20. Recommendation [ITU-R BS.1660](https://www.itu.int/rec/R-REC-BS.1660/recommendation.asp?lang=en&parent=R-REC-BS.1660-7-201510-I). [↑](#footnote-ref-20)
21. See Recommendation ITU-R P.1546-6, Annex 5 § 9. [↑](#footnote-ref-21)
22. Refer to Recommendation [ITU-R P.1546](http://www.itu.int/rec/R-REC-P.1546/en). The same as the value provided in GE06. [↑](#footnote-ref-22)
23. For Region 1 and the Islamic republic of Iran except the territory of Mongolia the use of the band 470‑694 MHz is subject to the GE06 agreement. [↑](#footnote-ref-23)
24. Pixel is a small area of typically about 100 m × 100 m where the percentage of covered receiving locations is indicated. [↑](#footnote-ref-24)