|  |
| --- |
| **Recommendation ITU-R SA.1414-1**  **(12/2013)** |
| **Characteristics of data relay  satellite systems** |
| **SA Series**  **Space applications and meteorology** |

Foreword

The role of the Radiocommunication Sector is to ensure the rational, equitable, efficient and economical use of the radio-frequency spectrum by all radiocommunication services, including satellite services, and carry out studies without limit of frequency range on the basis of which Recommendations are adopted.

The regulatory and policy functions of the Radiocommunication Sector are performed by World and Regional Radiocommunication Conferences and Radiocommunication Assemblies supported by Study Groups.

# Policy on Intellectual Property Right (IPR)

ITU-R policy on IPR is described in the Common Patent Policy for ITU-T/ITU-R/ISO/IEC referenced in Annex 1 of Resolution ITU-R 1. Forms to be used for the submission of patent statements and licensing declarations by patent holders are available from <http://www.itu.int/ITU-R/go/patents/en> where the Guidelines for Implementation of the Common Patent Policy for ITU‑T/ITU‑R/ISO/IEC and the ITU-R patent information database can also be found.

|  |  |
| --- | --- |
| Series of ITU-R Recommendations  (Also available online at <http://www.itu.int/publ/R-REC/en>) | |
| **Series** | Title |
| **BO** | Satellite delivery |
| **BR** | Recording for production, archival and play-out; film for television |
| **BS** | Broadcasting service (sound) |
| **BT** | Broadcasting service (television) |
| **F** | Fixed service |
| **M** | Mobile, radiodetermination, amateur and related satellite services |
| **P** | Radiowave propagation |
| **RA** | Radio astronomy |
| **RS** | Remote sensing systems |
| **S** | Fixed-satellite service |
| **SA** | **Space applications and meteorology** |
| **SF** | Frequency sharing and coordination between fixed-satellite and fixed service systems |
| **SM** | Spectrum management |
| **SNG** | Satellite news gathering |
| **TF** | Time signals and frequency standards emissions |
| **V** | Vocabulary and related subjects |

|  |
| --- |
|  |

|  |
| --- |
| ***Note***: *This ITU-R Recommendation was approved in English under the procedure detailed in Resolution ITU-R 1.* |

*Electronic Publication*

Geneva, 2014

© ITU 2014

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without written permission of ITU.

RECOMMENDATION ITU-R SA.1414-1

Characteristics of data relay satellite systems

(Question ITU-R 118/7)

(1999-2013)

Scope

This Recommendation provides parameters for data relay satellite (DRS) systems worldwide to be used as guidance for deriving sharing criteria and coordination thresholds.

Rec. ITU-R SA.1414

The ITU Radiocommunication Assembly,

considering

a)that data relay satellite (DRS) systems operate as described in Recommendation ITU‑R SA.1018 – Hypothetical reference system for systems comprising data relay satellites in the geostationary orbit and user spacecraft in low-Earth orbits;

b) that there is an increase in mission requirements and in space research activity conducted particularly in low-Earth orbit;

c) that DRS provide support to many programmes/missions in the space research service and are vital to supporting both manned and unmanned space research telecommunications;

d) that it is necessary to establish relevant criteria for sharing between DRS systems and other services operating in co-frequency bands;

e) that the technical characteristics of representative DRS systems need to be considered in order to derive relevant sharing criteria,

recommends

**1** that the characteristics of DRS systems, as described in Annex 1, may be used in interference sharing studies;

**2** that the information provided in Annex 1 should also be used as guidance for deriving sharing criteria and coordination thresholds as appropriate for DRS systems.

Annex 1  
  
Characteristics of existing Data Relay Satellite (DRS) systems

TABLE 1

Forward Earth-to-DRS feeder link characteristics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Transmitting earth station* | | | | | |
| Network | Russian Federation | United States of America | Europe | Japan | China |
| Location | Russian Federation(1) | United States of America(1) | Europe | Japan | China |
| Frequency range (GHz) | 14.5-15.34  selectable | 14.6-15.25 selectable | 28.6-29.8 selectable | 29.5-31 selectable | 29.4-30.2 selectable |
| Link description | Forward feeder-links  Ku-band(5) | Composite(2) | Decentralized(3) | Decentralized (3), (4) | Composite(7) |
| Transmission rate | ≤ 90 Mbit/s | ≤ 25 Mbit/s | ≤ 10 Mbit/s | ≤ 50 Mbit/s | ≤ 100 Mbit/s |
| Modulation | QPSK/SSM(6), QPSK | PSK | PSK | | |
| Polarization | Left-hand circular | Linear | Linear | Circular | Linear |
| Antenna size (m) | 13.1 | 18.3 | 3 and 9 | 5, 9.2 and 13 | 3, 12 and 15 |
| Tx antenna gain (dBi) | 63.3 | 66.4 | 57.6 and 67.6 | 63, 68.2  and 71.4 | 56.9, 68.2 and 70.1 |
| Tx antenna radiation pattern | Rec. ITU-R S.580 | RR Appendix 8, Annex III | | | |
| Necessary bandwidth (MHz) | ≤ 80 per channel | 650 (composite) | ≤ 100 | ≤ 978 (composite) | ≤ 800 (composite) |
| Maximum power spectral density (dB(W/Hz)) | –52.8 | –58 | –38 | –32.5 | –47 |
| Maximum e.i.r.p. spectral density (dB(W/Hz)) | 10.5 | 8.8 | 19.6 | 38.9 | 23.1 |
| *Receiving DRS* | | | | | |
| Orbital locations | 160W, 16W,  95E, 167E | Rec. ITU-R SA.1275 or Rec. ITU-R SA.1276 | | | |
| Antenna size (m) | 0.6 | 1.8 | 0.4 | 2.0 | 1.5 |
| Rx antenna gain (dBi) | 36 | 47.0 | 40.2 | 53 | 49.5 |
| Rx antenna radiation pattern | Rec. ITU-R S.672 | | | | |
| System noise temperature (K) | 550 | 977 | 1 305 | 890 and 579 | 1 318 |
| Link availability (%) | 99.9 | 99.9 | 99.9 | 99.9 | 99.9 |
| Interference criterion | Rec. ITU-R SA.1155 | | | | |
| (1) The earth stations for the Russian Federation network are located within the territory of the Russian Federation. The earth stations for the United States of America network are located in White Sands (New Mexico), Blossom Point (Maryland) and Guam. The coordinates of the stations are: 32.5° N, 106.60° W for White Sands; 38.43° N, 77.08° W for Blossom Point; and 13.62° N, 144.86° E for Guam.  (2) The composite link for the United States of America network is composed of seven channels: One DRS command and ranging channel, one DRS pilot tone signal, one S-band (2 GHz) multiple access (S‑MA) link, two S‑band single access (S-SA) links and two Ku-band (14/11 GHz and 30/20 GHz) single access (K-SA) links.  (3) The European DRS ground system consists of 12 earth stations, including the TT&C earth station, located in different countries within Europe. The earth station communicates with the DRS through its European coverage antenna.  (4) The Japanese network employs a decentralized link concept that permits independent forward feeder links from different earth stations.  (5) The Russian Federation DRS employs several independent forward feeder-links, including S-band (2 GHz) multiple access (S‑MA) links, S‑band single access (S-SA) links, Ku-band single access (Ku-SA) links and differential correction and monitoring system links that are augmented for the GLONASS system (GLONASS/SDCM).  (6) SSM: Spread-spectrum modulation.  (7) The Chinese networks implement a composite link concept that permits forward feeder links from different earth stations. | | | | | |

TABLE 2

Forward DRS-to-spacecraft link characteristics

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Transmitting DRS* | | | | | | | | | | | | | | |
| Network | Russian Federation | China | United  States of America | Europe | Japan | United States of America | China | Russian Federation | Russian Federation | United States of America | Europe | Japan | United States of America | China |
| Orbital locations | 16W, 95E, 167E | Rec. ITU-R SA.1275 or Rec. ITU-R SA.1276 | | | | | | 16W, 95E, 167E | 160W, 16W, 95E, 167E | Rec. ITU-R SA.1275 or Rec. ITU-R SA.1276 | | | | |
| Frequency range (GHz) | 2.025- 2.110(3) | 2.090- 2.098 | 2.103- 2.110 | 2.025-2.110(1) | | | | | 13.4-13.8 | 13.750-13.800 | 22.55-23.55 | | | |
| Link description | Multiple access (S-MA) links | | | Single access (S-SA) links | | | | | Single Access (Ku-SA) links | | Single Access (Ka-SA) links | | | |
| Transmission rate (bit/s) | ≤ 1 kbit/s | ≤ 300 kbit/s 3 Mcps | | ≤ 1 Mbit/s | ≤ 6 Mbit/s | ≤ 300 kbit/s 3 Mcps | ≤ 300 kbit/s 3 Mcps | ≤ 64  kbit/s | ≤ 40 Mbit/s | ≤ 25  Mbit/s | ≤ 10 Mbit/s | ≤ 50 Mbit/s | ≤ 25 Mbit/s | ≤ 100 Mbit/s |
| Modulation | QPSK/SSM(2) | PSK | SQPN/PSK(2) | | | | PSK | QPSK/SSM(2) | QPSK | PSK | | | | |
| Polarization | RHC | LHC | LHC | Circular | | | | RHC | RHC | Circular | | | | |
| Antenna size (m) | Phased array | | Phased array | 2.8 | 3.6 | 4.9 | 4.2 | 4 | 4 | 4.9 | 2.8 | 3.6 | 4.9 | 4.2 |
| Tx antenna gain (dBi) | 14.3 | 26 | 26.0 | 34 | 36.4 | 36.0 | 35 | 35.0 | 51.8 | 51.2 | 53.4 | 57.4 | 54.7 | 56.5 |
| Tx antenna radiation pattern | Rec. ITU-R S.672 | Rec. ITU-R S.672 | Rec. ITU-R S.672 | | | | | | | | | | | |
| Necessary bandwidth (MHz) | ≤ 6 | ≤ 8 | ≤ 6 | ≤ 6 | 30 | 6 | 20 | 6 | 40 | 50 | 60 | ≤ 150 | 50 | ≤ 100 |
| Maximum power spectral density (dB(W/Hz)) | –52.5 | –46 | –51.8 | –54.7 | –44.5 | –55.3 | –49.9 | –56.4 | –66.6 | –79.7 | –65.1 | –49.5 | –68.7 | –64 |
| Maximum e.i.r.p. spectral density (dB(W/Hz)) | –38.2 | –20 | –25.8 | –20.7 | –8.1 | –19.3 | –14.9 | –21.4 | –14.8 | –28.5 | –11.7 | –7.9 | –14.0 | –7.5 |
| LHC – Left-hand circular; RHC – right-hand circular. | | | | | | | | | | | | | | |

TABLE 2 (*end*)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Receiving spacecraft* | | | | | | | | | | | | | | |
| Network | Russian Federation | China | United States of America | Europe | Japan | United States of America | Russian Federation | China | Russian Federation | United States of America | Europe | Japan | United States of America | China |
| Orbital locations | Mainly low-Earth orbit | | | | | | | | | | | | | |
| Frequency range (GHz) | 2.025-2.110(3) | 2.090-2.098 | 2.103-2.110 | 2.025-2.110(1) | | | | | 13.4-13.8 | 13.750-13.800 | 22.55-23.55 | | | |
| Antenna size (m) | Omnidirectional,  arrays | | | Omnidirectional, arrays, parabolic = ≤ 1.5 | | | | Omnidi-rectional, arrays, parabolic  ≤ 0.8 | ≤ 1.2 | ≤  | ≤ 1.3 |  | ≤ 1.3 | ≤ 0.8 |
| Rx antenna gain (dBi) | ≤ 1.5 / ≤ 7.2 | ≤  | ≤ 1.5 | ≤ 27.3 | ≤ 27.1 | ≤ 27.3 | ≤ 11 | ≤ 15 | ≤ 40.8 | ≤  | ≤ 47 | ≤ 48.9 | ≤ 47 | ≤ 43 |
| Rx antenna radiation pattern |  | Rec. ITU-R S.672 for high gain antenna | | | | | | | Rec. ITU-R S.672 | | | | | |
| System noise temperature (K) |  |  |  |  |  |  |  | 600 |  | 1 000 |   |  |   |   |
| Required *Eb*/*N*0 (dB) | 10.6 | 9.5 | –9.5 | 9.5 | 10.5 | 9.5 | 10.6 | 9.5 | 10.6 | 9.5 | 9.5 | 10.8 | 9.5 | 9.5 |
| Required BER | 1 × 10–6 | 1 × 10–6 | 1 × 10–5 | 1 × 10–6 | 1 × 10–6 | 1 × 10–5 | 1 × 10–6 | 1 × 10–6 | 1 × 10–6 | 1 × 10–5 | 1 × 10–6 | | 1 × 10–5 | 1 × 10–6 |
| Link reliability (%) | 99.9 | 99.9 | 99.99 | 99.9 | 99.9 | 99.99 | 99.9 | 99.9 | 99.9 | 99.9 | 99.9 | | 99.9 | 99.9 |
| Interference criterion | Rec. ITU-R SA.1155 | | | | | | | | | | | | | |
| SQPN: Staggered quadriphase pseudo-random noise; SSM: Spread-spectrum modulation.  (1) Transmit frequency is selectable in 5 MHz steps, 500 × 221/240 kHz steps for the Russian Federation DRS, 1 MHz steps for Chinese DRS.  (2) Signals with low data rate transmissions will be spread by a pseudo-random noise code so as to meet pfd limits.  (3) For the Russian Federation DRS transmit frequency is selectable in 500 × 221/240 kHz steps. | | | | | | | | | | | | | | |

TABLE 3

Return spacecraft-to-DRS link characteristics

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Transmitting spacecraft* | | | | | | | | | | | | | | | |
| Network | Russian Federation | China | United States of America | Europe | Japan | United States of America | China | Russian Federation | Russian Federation | United States of America | Europe | Japan | United States of America | | China |
| Orbital locations | Mainly low-Earth orbit | | | | | | | | | | | | | | |
| Frequency range (GHz) | 2.200-2.290(3) | 2.270-2.278 | 2.284-2.291 | 2.200-2.290(1) | | | | | 14.76-15.34 | 14.891-15.116 | 25.25-27.50 | | | | |
| Link description | Multiple access (S-MA) links | | | Single access (S-SA) links | | | | | Single access (Ku-SA) links | | Single access (Ka-SA) links | | | | |
| Transmission rate | ≤ 1 kbit/s | ≤ 300 kbit/s 3 Mcps | ≤ 3 Mbit/s | ≤ 1 Mbit/s | ≤ 12 Mbit/s | ≤ 6 Mbit/s | ≤ 2 Mbit/s | ≤ 64 kbit/s | ≤ 90 Mbit/s | ≤ 300 Mbit/s | ≤ 150 Mbit/s | ≤ 300 Mbit/s | ≤ 800 Mbit/s | ≤ 600 Mbit/s | |
| Modulation | QPSK/SSM | PSK | SQPN/PSK(2) | | | | PSK | QPSK/SSM | QPSK | PSK | | | | | |
| Polarization | RHC | LHC | LHC | Circular | | | | RHC | RHC | Circular | | | | | |
| Antenna size (m) | Omnidirectional, arrays | | | Omnidirectional, arrays, parabolic   1.5 | | | Omnidi-rectional, arrays, parabolic = ≤ 0.8 | Omnidi-rectional, arrays, parabolic  = ≤ 1.5 | ≤ 1.2 | ≤ 1.5 | | ≤ 1.9 | ≤ 1.5 | ≤ 0.8 | |
| Tx antenna gain (dBi) | ≤ 1.5 / 7.2 | ≤ 11 | ≤ 15 | ≤ 27.3 | ≤ 27.6 | ≤ 27.3 | ≤ 15 | ≤ 11 | ≤ 42.2 | ≤  | ≤ 47 | ≤ 49.7 | ≤ 47 | ≤ 44.5 | |
| Tx antenna radiation pattern | Rec. ITU-R S.672 for high gain antenna | | | | | | | | Rec. ITU-R S.672 | | | | | | |
| Necessary bandwidth (MHz) | 6 | 8 | 6 | ≤ 6 | 20 | 6 | 20 | 6 | ≤ 80 per channel | ≤ 225 | ≤ 300 | ≤ 300 | ≤ 650 | ≤ 600 | |
| Maximum power spectral density (dB(W/Hz)) | –55.8 | –46 | –60.8 | –51 | –55.7 | –60.8 | –46 | 55.8 | –71.5 | –73.5 | –65.1 | –58.8 | –67.5 | –50 | |
| Maximum e.i.r.p. spectral density (dB(W/Hz)) | Compliant with pfd limits | | | | | | | | –29.3 | –30.5 | –23 | –9.1 | –20.5 | –5.5 | |

TABLE 3 (*end*)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Receiving DRS* | | | | | | | | | | | | | | |
| Network | Russian Federation | China | United States of America | Europe | Japan | United States of America | China | Russian Federation | Russian Federation | United States of America | Europe | Japan | United States of America | China |
| Orbital locations | 16W, 95E, 167E | Rec. ITU-R SA.1275  or Rec. ITU-R SA.1276 | | | | | | 16W, 95E, 167E | 160W, 16W, 95E, 167E | Rec. ITU-R SA.1275 or Rec. ITU-R SA.1276 | | | | |
| Frequency range (GHz) | 2.200-2.290(1) | 2.270- 2.278 | 2.284-2.291 | 2.200-2.290(1) | | | | | 14.76-15.34 | 14.891-15.116 | 25.25-27.50 | | | |
| Antenna size (m) | Horn | Phased array | | 2.8 | 3.6 | 4.9 | 4.2 | 4 | 4 | 4.9 | 2.8 | 3.6 | 4.9 | 4.2 |
| Rx antenna gain (dBi) | 14.8 | 27 | 30.0 | 34.7 | 37.2 | 36.8 | 36.5 | 35.7 | 52.6 | 52.6 | 53.4 | 58.8 | 55.9 | 57.5 |
| Rx antenna radiation pattern | Rec. ITU-R S.672 | Rec. ITU-R S.672 | Rec. ITU-R S.672 | | | | | | | | | | | |
| System noise temperature (K) | 450 | 741 | 478 | 590 | 404 | 537 | 741 | 550 | 550 | 661 | 1 305 | 475 | 870 | 1 000 |
| Link reliability (%) | 99.9 | 99.9 | 99.99 | | 99.9 | 99.99 | 99.9 | 99.9 | 99.9 | 99.9 | 99.9 | | 99.9 | 99.9 |
| Interference criterion | Rec. ITU-R SA.1155 | | | | | | | | | | | | | |
| (1) Transmit frequency is selectable in 5 MHz steps for United States of America DRS, 100 kHz steps for Japanese DRS, 500 kHz for the Russian Federation DRS, 1 MHz steps for Chinese DRS.  (2) Signals with low data rate transmissions will be spread by a pseudo-random noise code so as to meet pfd limits. | | | | | | | | | | | | | | |

TABLE 4

Return DRS-to-Earth feeder link characteristics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Transmitting DRS* | | | | | |
| Network | Russian Federation | United States of America | Europe | Japan | China |
| Orbital locations | 160W, 16W,  95E, 167E | Rec. ITU-R SA.1275 or Rec. ITU-R SA.1276 | | | |
| Frequency range (GHz) | 10.7-10.95,  11.45-11.7,  12.5-12.75 | 13.4-14.05 | 18.1-21.2 | 19.7-21.2 | 18.9-21.2 |
| Link description | Ku-band  (14/11 GHz)  return feeder | Ku-band (14/11 GHz)  return feeder | Ka-band (30/20 GHz) return feeder | | |
| Transmission rate (Mbit/s) | ≤ 150(3) | (1) | (2) | (2) | (4) |
| Modulation | QPSK, QPSK/SSM | PSK | | SQPN/PSK | PSK |
| Polarization | RHC | Linear | | Circular | Linear |
| Antenna size (m) | 0.6 | 2 | 0.4 | 2.0 | 1.5 |
| Tx antenna gain (dBi) | 34.3 | 44.8 | 40.2 | 49.5 | 46.4 |
| Tx antenna radiation pattern | Rec. ITU-R S.672 | | | | |
| Necessary bandwidth (MHz) | ≤ 150 per channel | 650 (composite), 225 (dedicated) | ≤ 300 | 839 | ≤ 2  (composite) |
| Maximum power spectral density (dB(W/Hz)) | –57.5 | –58.6 | –61 | –40.9 | –57.1 |
| Maximum e.i.r.p. density (dB(W/Hz)) | –23.2 | –13.8 | –20.8 | 8.6 | –10.7 |
| *Receiving earth station* | | | | | |
| Location | Russian Federation | United States of America | Europe | Japan | China |
| Antenna size (m) | 13.1 | 18.3 | 3, 9 | 5, 9.2 and 13 | 3, 12 and 15 |
| Rx antenna gain (dBi) | 61.3 | 65.5 | 54, 63.9 | 59.5, 67.7 | 53.4, 65.5  and 67.1 |
| Rx antenna radiation pattern | Rec. ITU-R S.580 | RR Appendix 8, Annex III | | | |
| System noise  temperature (K) | 320 | 300 | 795 | 200 | 330 |
| Link availability (%) | 99.9 | 99.9 | 99.9 | | |
| Interference criterion | Rec. ITU-R SA.1155, Rec. ITU-R S.741 | Rec. ITU-R SA.1155 | | | |
| (1) The United States of America DRS transmits a dedicated and a composite link. Transmission rate for the dedicated link is 300 Mbit/s, for the composite link the transmission rate is on the order of 800 Mbit/s.  (2) The European and Japanese networks employ a decentralized link concept that permits independent return feeder links to different earth station.  (3) The Russian Federation DRS transmits several independent return feeder links within the indicated frequency range with transmission rates ≤ 150 Mbits/s.  (4) The Chinese networks implement a composite link concept that permits return feeder links to different earth stations. | | | | | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_