|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 2 toDocument 124-E** |
|  | **16 October 2015** |
|  | **Original: Spanish** |
|  |
| Ecuador |
| Proposals for the work of the conference |
|  |
| Agenda item 8 |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC‑07)**;

Introduction

In Ecuador, the entire frequency band 430-440 MHz is used exclusively by the fixed service on a primary basis.

In letter 60(TSD/SSD)O-2015-002994 of 30 July 2015, the Radiocommunication Bureau (BR) replied to the question asked by the Administration of Ecuador concerning the procedure for modifying or changing footnotes.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD EQA/124A2/1

410-460 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 430-432AMATEURRADIOLOCATION | 430-432 RADIOLOCATION Amateur |
| 5.271 5.272 5.273 5.2745.275 5.276 5.277 |  5.271 MOD 5.276 5.278 5.279 |
| 432-438AMATEURRADIOLOCATIONEarth exploration-satellite(active) 5.279A | 432-438 RADIOLOCATION Amateur Earth exploration-satellite (active) 5.279A |
| 5.138 5.271 5.272 5.2765.277 5.280 5.281 5.282 |  5.271 MOD 5.276 5.278 5.279 5.281 5.282 |

MOD EQA/124A2/2

410-460 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 438-440AMATEURRADIOLOCATION | 438-440 RADIOLOCATION Amateur |
| 5.271 5.273 5.274 5.2755.276 5.277 5.283 |  5.271 MOD 5.276 5.278 5.279 |

**Reasons:** In Ecuador, the frequency bands 430-435 MHz and 438-440 MHz are used exclusively by the fixed service on a primary basis and are not used by the mobile service, except aeronautical mobile.

MOD EQA/124A2/3

5.276 *Additional allocation:*in Afghanistan, Algeria, Saudi Arabia, Bahrain, Bangladesh, Brunei Darussalam, Burkina Faso, Djibouti, Egypt, the United Arab Emirates, Ecuador, Eritrea, Ethiopia, Greece, Guinea, India, Indonesia, Iran (Islamic Republic of), Iraq, Israel, Italy, Jordan, Kenya, Kuwait, Libya, Malaysia, Niger, Nigeria, Oman, Pakistan, the Philippines, Qatar, the Syrian Arab Republic, the Dem. People’s Rep. of Korea, Singapore, Somalia, Sudan, Switzerland, Tanzania, Thailand, Togo, Turkey and Yemen, the band 430-440 MHz is also allocated to the fixed service on a primary basis and the bands 430-435 MHz and 438-440 MHz are also allocated, except in Ecuador, to the mobile, except aeronautical mobile, service on a primary basis.    (WRC‑15)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_