|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Document 128-E** |
|  | **19 October 2015** |
|  | **Original: English** |
|  |
| Benin (Republic of)/Burkina Faso/Côte d'Ivoire (Republic of)/Ghana/Guinea (Republic of)/Mali (Republic of)/Niger (Republic of the)/Nigeria (Federal Republic of)/Senegal (Republic of)/Sierra Leone/Togolese Republic |
| Proposals for the work of the conference |
|  |
| Agenda item 1.1 |

1.1 to consider additional spectrum allocations to the mobile service on a primary basis and identification of additional frequency bands for International Mobile Telecommunications (IMT) and related regulatory provisions, to facilitate the development of terrestrial mobile broadband applications, in accordance with Resolution **233 (WRC‑12)**;

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD BEN/BFA/CTI/GHA/GUI/MLI/NGR/NIG/SEN/SRL/TGO/128/1

5.384A The bands, or portions of the bands, 1 710-1 885 MHz, 2 300-2 400 MHz, 2 500-2 690 MHz and 4 800-4 990 MHz are identified for use by administrations wishing to implement International Mobile Telecommunications (IMT) in accordance with Resolution **223 (Rev.WRC‑07)**\*. This identification does not preclude the use of these bands by any application of the services to which they are allocated and does not establish priority in the Radio Regulations.     (WRC‑15)

MOD BEN/BFA/CTI/GHA/GUI/MLI/NGR/NIG/SEN/SRL/TGO/128/2

4 800-5 570 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 4 800-4 990 FIXED MOBILE 5.440A 5.442  Radio astronomy 5.149 5.339 5.443 MOD 5.384A |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_