|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 5 toDocument 24(Add.13)-E** |
|  | **20 September 2019** |
|  | **Original: English** |
|  |
| Asia-Pacific Telecommunity Common Proposals |
| PROPOSALS FOR THE WORK OF THE CONFERENCE |
|  |
| Agenda item 1.13 |

1.13 to consider identification of frequency bands for the future development of International Mobile Telecommunications (IMT), including possible additional allocations to the mobile service on a primary basis, in accordance with Resolution **238 (WRC-15)**;

Part 5 - Frequency band 47-47.2 GHz

Introduction

This document presents the APT Common Proposal for the frequency band 47-47.2 GHz under WRC-19 agenda item 1.13.

Proposals

APT Members support no change to the RR in this frequency band.

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

NOC ACP/24A13A5/1

40-47.5 GHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 40-40.5 EARTH EXPLORATION-SATELLITE (Earth-to-space) FIXED FIXED-SATELLITE (space-to-Earth) 5.516B MOBILE MOBILE-SATELLITE (space-to-Earth) SPACE RESEARCH (Earth-to-space) Earth exploration-satellite (space-to-Earth) |
| 40.5-41FIXEDFIXED-SATELLITE (space-to-Earth)BROADCASTINGBROADCASTING-SATELLITEMobile5.547 | 40.5-41FIXEDFIXED-SATELLITE (space-to-Earth) 5.516BBROADCASTINGBROADCASTING-SATELLITEMobileMobile-satellite (space-to-Earth)5.547 | 40.5-41FIXEDFIXED-SATELLITE (space-to-Earth)BROADCASTINGBROADCASTING-SATELLITEMobile5.547 |
| 41-42.5 FIXED FIXED-SATELLITE (space-to-Earth) 5.516B BROADCASTING BROADCASTING-SATELLITE Mobile 5.547 5.551F 5.551H 5.551I |
| 42.5-43.5 FIXED FIXED-SATELLITE (Earth-to-space) 5.552 MOBILE except aeronautical mobile RADIO ASTRONOMY 5.149 5.547 |
| 43.5-47 MOBILE 5.553 MOBILE-SATELLITE RADIONAVIGATION RADIONAVIGATION-SATELLITE 5.554 |
| 47-47.2 AMATEUR AMATEUR-SATELLITE |
| 47.2-47.5 FIXED FIXED-SATELLITE (Earth-to-space) 5.552 MOBILE 5.552A |

**Reasons:** APT Members agreed not to support IMT identification in the frequency band 47‑47.2 GHz at WRC-19.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_