|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19) Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 20 to Document 33-E** |
|  | **30 September 2019** |
|  | **Original: French** |
|  | |
| France | |
| Proposals for the work of the conference | |
|  | |
| Agenda item 8 | |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC-07)**;

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

MOD F/33A20/1

5.349 *Different category of service*:  in Saudi Arabia, Azerbaijan, Bahrain, Cameroon, Egypt, Iran (Islamic Republic of), Iraq, Israel, Kazakhstan, Kuwait, The Former Yugoslav Republic of Macedonia, Lebanon, Morocco, Qatar, Syrian Arab Republic, Kyrgyzstan, Turkmenistan and Yemen, the allocation of the band 1 525‑1 530 MHz to the mobile, except aeronautical mobile, service is on a primary basis (see No. **5.33**).     (WRC‑19)

**Reasons:** It is no longer necessary to refer to France in this footnote.

MOD F/33A20/2

5.352A In the frequency band 1 525-1 530 MHz, stations in the mobile-satellite service, except stations in the maritime mobile-satellite service, shall not cause harmful interference to, or claim protection from, stations of the fixed service in Algeria, Saudi Arabia, Egypt, , Guinea, India, Israel, Italy, Jordan, Kuwait, Mali, Morocco, Mauritania, Nigeria, Oman, Pakistan, the Philippines, Qatar, Syrian Arab Republic, Viet Nam and Yemen notified prior to 1 April 1998.     (WRC‑19)

**Reasons:** It is no longer necessary to refer to France in this footnote.

MOD F/33A20/3

5.359 *Additional allocation:* in Germany, Saudi Arabia, Armenia, Azerbaijan, Belarus, Benin, Cameroon, the Russian Federation, , Georgia, Guinea, Guinea-Bissau, Jordan, Kazakhstan, Kuwait, Lithuania, Mauritania, Uganda, Uzbekistan, Pakistan, Poland, the Syrian Arab Republic, Kyrgyzstan, the Dem. People’s Rep. of Korea, Romania, Tajikistan, Tunisia, Turkmenistan and Ukraine, the frequency bands 1 550-1 559 MHz, 1 610-1 645.5 MHz and 1 646.5-1 660 MHz are also allocated to the fixed service on a primary basis. Administrations are urged to make all practicable efforts to avoid the implementation of new fixed-service stations in these frequency bands.     (WRC‑19)

**Reasons:** It is no longer necessary to refer to France in this footnote.

MOD F/33A20/4

5.495 *Additional allocation:* in Greece, Monaco, Montenegro, Uganda, Romania and Tunisia, the frequency band 12.5-12.75 GHz is also allocated to the fixed and mobile, except aeronautical mobile, services on a secondary basis.     (WRC‑19)

**Reasons:** It is no longer necessary to refer to France in this footnote.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_