|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 20 toDocument 85-E** |
|  | **7 October 2019** |
|  | **Original: English** |
|  |
| Iran (Islamic Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 8 |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC-07)**;

Introduction

Resolution **26 (Rev.WRC-07)** urges administrations to review periodically footnotes in Article **5** of the Radio Regulations (RR) and to propose the deletion of their country footnotes or their country names from footnotes, as appropriate.

The Islamic Republic of Iran has reviewed the relevant footnotes of the table of frequency allocations in RR Article **5** and proposes to delete its name from RR No. **5.67B** related to the band 135.7-137.8 kHz and RR No. **5.401** related to the band 2 483.5-2 500 MHz.

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD IRN/85A20/1

5.67B The use of the band 135.7-137.8 kHz in Algeria, Egypt, Iraq, Lebanon, Syrian Arab Republic, Sudan, South Sudan and Tunisia is limited to the fixed and maritime mobile services. The amateur service shall not be used in the above-mentioned countries in the band 135.7-137.8 kHz, and this should be taken into account by the countries authorizing such use.    (WRC‑19)

**Reasons:** The condition mentioned in the footnote are no longer required in the Islamic Republic of Iran.

MOD IRN/85A20/2

5.401 In Angola, Australia, Bangladesh, China, Eritrea, Ethiopia, India, Lebanon, Liberia, Libya, Madagascar, Mali, Pakistan, Papua New Guinea, Syrian Arab Republic, Dem. Rep. of the Congo, Sudan, Swaziland, Togo and Zambia, the frequency band 2 483.5-2 500 MHz was already allocated on a primary basis to the radiodetermination-satellite service before WRC‑12, subject to agreement obtained under No. **9.21** from countries not listed in this provision. Systems in the radiodetermination-satellite service for which complete coordination information has been received by the Radiocommunication Bureau before 18 February 2012 will retain their regulatory status, as of the date of receipt of the coordination request information.     (WRC‑19)

**Reasons:** Since, there is not any complete coordination information already submitted by 18 February 2012, Therefore the mentioning of the Islamic Republic of Iran in footnote No. **5.401** is no longer required.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_