Recommendation ITU-R BS.1285-1

(05/2023)

BS Series: Broadcasting service (sound)

Pre-selection methods for the subjective assessment of small impairments in audio systems

Foreword

The role of the Radiocommunication Sector is to ensure the rational, equitable, efficient and economical use of the radio-frequency spectrum by all radiocommunication services, including satellite services, and carry out studies without limit of frequency range on the basis of which Recommendations are adopted.

The regulatory and policy functions of the Radiocommunication Sector are performed by World and Regional Radiocommunication Conferences and Radiocommunication Assemblies supported by Study Groups.

# Policy on Intellectual Property Right (IPR)

ITU-R policy on IPR is described in the Common Patent Policy for ITU-T/ITU-R/ISO/IEC referenced in Resolution ITU‑R 1. Forms to be used for the submission of patent statements and licensing declarations by patent holders are available from <http://www.itu.int/ITU-R/go/patents/en> where the Guidelines for Implementation of the Common Patent Policy for ITU‑T/ITU‑R/ISO/IEC and the ITU-R patent information database can also be found.

|  |  |
| --- | --- |
| Series of ITU-R Recommendations  (Also available online at <https://www.itu.int/publ/R-REC/en>) | |
| **Series** | Title |
| **BO** | Satellite delivery |
| **BR** | Recording for production, archival and play-out; film for television |
| **BS** | **Broadcasting service (sound)** |
| **BT** | Broadcasting service (television) |
| **F** | Fixed service |
| **M** | Mobile, radiodetermination, amateur and related satellite services |
| **P** | Radiowave propagation |
| **RA** | Radio astronomy |
| **RS** | Remote sensing systems |
| **S** | Fixed-satellite service |
| **SA** | Space applications and meteorology |
| **SF** | Frequency sharing and coordination between fixed-satellite and fixed service systems |
| **SM** | Spectrum management |
| **SNG** | Satellite news gathering |
| **TF** | Time signals and frequency standards emissions |
| **V** | Vocabulary and related subjects |

|  |
| --- |
|  |

|  |
| --- |
| ***Note***: *This ITU-R Recommendation was approved in English under the procedure detailed in Resolution ITU-R 1.* |

*Electronic Publication*

Geneva, 2023

© ITU 2023

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without written permission of ITU.

RECOMMENDATION ITU-R BS.1285-1

Pre-selection methods for the subjective assessment  
of small impairments in audio systems

(1997-2023)

Scope

This Recommendation describes pre-selection methods for the subjective assessment of small impairments in audio systems.

Keywords

Pre-selection method, audio quality, subjective assessment, listening test

The ITU Radiocommunication Assembly,

considering

*a)* that Recommendations ITU-R BS.1116, ITU-R BT.500 and ITU-R BS.1284 have established some methods for assessing the subjective quality of audio and video systems;

*b)* that subjective listening tests permit assessment of the degree of annoyance caused to the listener by any impairment of the wanted signal during its transmission between the source and the listener;

*c)* that classical objective methods may not be adequate for assessing advanced audio coding schemes and that perceptual objective assessment methods are being developed for testing the sound quality of sound systems;

*d)* that the use of standardized methods is important for the exchange, compatibility and correct evaluation of the test data;

*e)* that the introduction of new advanced digital audio systems exploiting psycho-acoustic properties, especially with small impairments, requires advancements in subjective assessment methods;

*f)* that Recommendation ITU-R BS.1116 has established a method for the evaluation of the sound quality of sound systems which introduce small impairments;

*g)* that the detailed procedures of Recommendation ITU-R BS.1116 can be time-consuming and comparatively expensive to carry out and therefore a pre-selection method for rejecting systems which introduce large impairments is desirable,

recommends

that the testing, evaluation and reporting procedures given in Annex 1 should be used as a means of distinguishing between those audio systems which introduce large impairments and other systems.

Annex 1

# 1 General

This Annex is divided into the following sections, giving detailed requirements for various aspects of the tests:

1 General

2 Experimental design

3 Selection of the listening panel

4 Test method

5 Attributes

6 Programme material

7 Choice of reproduction devices

8 Listening conditions

9 Statistical analysis

10 Presentation of results

11 Contents of test report.

This Recommendation is based on Recommendation ITU-R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en). It differs mainly in the section referring to test method.

Recommendation ITU-R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en) – Methods for the subjective assessment of small impairments in audio systems including multichannel sound systems, is intended for the assessment of audio systems which introduce impairments that can be hard to detect. For that purpose, it is necessary to control as many of the test parameters as possible and to carry out a sufficient number of assessments to produce statistically reliable estimates of the impairments. The requirements of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en) are consequently stringent. The procedure is costly in time and effort and is unneces­sary if the systems under test produce significant impairments.

In order to avoid carrying out such tests unnecessarily, a pre-selection methodology that can reliably reject systems introducing large impairments is desirable. This reduction in the extent of the test method may reduce its sensitivity, but the method must still be capable of distinguishing between systems which introduce large impairments and those that do not.

# 2 Experimental design

In designing the tests, the considerations of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 2, should be taken into account.

# 3 Selection of the listening panel

For the selection of the listening panel, the considerations of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 3, should be taken into account.

However, to maximize the sensitivity of the test and minimize the number of trials required to obtain reliable results, the expert listeners should be thoroughly familiar with the types of impairment expected. That is, they should preferably be specialists in the assessment of the types of coding systems under test.

# 4 Test method

For the details of the test method, the general considerations of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 4, should be taken into account. As the test procedure is the most time-consuming aspect of Recommendation ITU-R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), it is by reduction of the test methodology that most savings in time and effort can be made. At present, the following methods can be recommended.

## 4.1 Assessment using headphones

If it can be shown that the systems under test can be properly assessed using headphone listening, then the assessments may be carried out by more than one subject at the same time. This excludes systems which inherently require the use of loudspeakers, any systems or tests which involve the acoustics of the listening environment and systems involving any spatial effects which cannot be properly reproduced by headphones.

Using subjects in groups, individual switching is not practical and it is not possible to randomize the order of presentation of stimuli for each test subject within a group. Between groups, different orders of presentation should be used. The principle of double-blind testing should be maintained.

The data analysis should be carried out according to Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 9, as far as is appropriate. The analysis should take into account the sub-division of the test subjects into groups.

## 4.2 Assessment using small numbers of expert listeners

The time taken by the test procedure can be reduced greatly by reducing the number of listeners. This is only practicable with expert listeners, who have previously demonstrated high levels of accuracy and consistency in similar tests.

The limited amount of data which might result from such tests may make useful statistical analysis impossible.

## 4.3 Further simplification of the test method

The test procedure may be further simplified by using a two-way comparison. In that way, the test subjects are required to make only one assessment between two signals, one of which is known to be the reference signal. The reference signal may be impaired and it may then be appropriate to use the seven-point comparison scale (see Recommendation ITU-R BS.1284 – Methods for the subjective assessment of sound quality – General requirements). It should be noted that such a method can give only a limited indication of the reliability of the subjects.

# 5 Attributes

Recommendation ITU‑R [[BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en)](https://www.itu.int/rec/R-REC-BS.1116/en), § 5, includes descriptions of the audio quality attributes that might be assessed, for monophonic, two-channel and multichannel stereophonic systems.

# 6 Programme material

For the selection of test programme material, the considerations of Recommendation ITU‑R [[BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en)](https://www.itu.int/rec/R-REC-BS.1116/en), § 6, should be followed.

# 7 Choice of reproduction devices

For the chosen reproduction devices, the considerations of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 7, should be followed.

# 8 Listening conditions

For the relevant listening conditions, the considerations of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 8, should be followed.

# 9 Statistical analysis

For the statistical analysis of the data, Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 9, should be followed as far as is appropriate.

It is important to note that, due to the methodology employed, the results from the pre-selection tests can only be used to determine whether or not to include or reject audio systems for subsequent formal tests. Only a statement about whether a system has “passed” or “failed” can be made. No further conclusions regarding the relative performances of the systems may be drawn from the results of the pre-selection tests.

The decision threshold should be set so that marginal systems are included in the “pass” category.

# 10 Presentation of results

For the presentation of the results, the considerations of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 10, should be taken into account as far as is appropriate.

The objective of the tests is simply to distinguish between systems that produce large impairments and those that do not. The final result will be simply a statement of whether a system has “passed” or “failed”.

# 11 Contents of test report

The contents of the test report should follow the considerations of Recommendation ITU‑R [BS.1116](https://www.itu.int/rec/R-REC-BS.1116/en), § 11, as far as is appropriate.